



U-Boot 2010.06 (Nov 06 2013 - 10:37:47)



Check spi flash controller v350... Found

Spi(cs1) ID: 0x01 0x20 0x18 0x03 0x01 0x00

Spi(cs1): Block:64KB Chip:16MB Name:"S25FL128P-1"

In:    serial

Out:   serial

Err:   serial

current hi352xx version 201306211132

current used inner phy

current used 512M mem

current used param offset 11111111111111111

current do_check_flash_boot_param

current prod net 100m

init gpio led setting

dev 0 set background color!

dev 2 set background color!

dev 0 opened!

dev 2 opened!

jpeg decoding ...

<<addr=0x80080000, size=0x171a8, vobuf=0x8fd00000>>

mmu_enable

<<imgwidth=480, imgheight=320, linebytes=960>>

decode success!!!!

dev 0 set background color!

dev 2 set background color!

dev 0 opened!

vo hd 0 end

dev 2 opened!

vo cvbs end

graphic layer 0 opened!

graphic layer 2 opened!

USB:   scanning bus for devices... 1 USB Device(s) found

0 Storage Device(s) found

start download process.

version: 3.0.3

(OK)

spi

(OK)

Block:64KB Chip:16MB*1 

ID:0x01 0x20 0x18 0x03 0x01 

Name:"S25FL128P-1"

(OK)

getinfo - print hardware information



(ERROR)

16384 KiB hi_sfc at 0:0 is now current device

(OK)


Erasing at 0x10000 --  25% complete.
Erasing at 0x20000 --  50% complete.
Erasing at 0x30000 --  75% complete.
Erasing at 0x40000 -- 100% complete.

(OK)


Writing at 0x10000 --  25% complete.
Writing at 0x20000 --  50% complete.
Writing at 0x30000 --  75% complete.
Writing at 0x40000 -- 100% complete.

(OK)

