const uint8_t SX_X[15]					=	"End SM         ";

const uint8_t SX_0[13]					=	"System       ";
const uint8_t SX_1[13]					=	"Partitions   ";
const uint8_t SX_2[13]					=	"Expanders    ";
const uint8_t SX_3[13]					=	"Zones        ";
const uint8_t SX_4[13]					=	"Outputs      ";
const uint8_t SX_5[13]					=	"Timers       ";
const uint8_t SX_6[13]					=	"GSM          ";

const struct {
	const uint8_t filling1[13];
	const uint8_t filling2[3];
} SX_7 = {										"Monitoring   ",
	{32,32,32}
};

const uint8_t SX_8[13]					=	"Telephones   ";

const struct {
	const uint8_t filling1[13];
	const uint8_t filling2[3];
	const uint8_t filling3[16];
} SX_9 = {										"AUDIO messag.",
	{32,32,32},
													"Double v.message"
};

const uint8_t SX_10[13]					=	"SMS messaging";
const uint8_t SX_11[12]					=	"SMS control ";
const uint8_t SX_12[12]					=	"Others      ";

const uint8_t SX_00[13]					=	"Service code";
const uint8_t SX_01[13]					=	"PERFECTA key";
const uint8_t SX_02[12]					=	"Factory set.";
const uint8_t SX_03[13]					=	"SM config   ";
const uint8_t SX_04[12]					=	"PERFECT.Soft";
const uint8_t SX_05[12]					=	"Remot.update";
const uint8_t SX_06[12]					=	"Time        ";
const uint8_t SX_09[12]					=	"Hide SM     ";

const uint8_t SX_061[12]				=	"DST        ";
const uint8_t SX_062[12]				=	"Summer from";
const uint8_t SX_063[12]				=	"Winter from";
const uint8_t SX_064[12]				=	"Timezone   ";
const uint8_t SX_065[12]				=	"RTC adjust.";

const struct {
	const uint8_t filling1[1];
	const uint8_t filling2[11];
} txt_065 = {{32},							"s/week     "
};

const uint8_t SX_Twy[12]				=	"Exit delay  ";

const uint8_t SX_WRN[12]				=	"Warn.delay  ";

const uint8_t SX_VRF[12]				=	"Verif.delay ";

const uint8_t SX_OPTS[13]				=	"Options     ";

const uint8_t SX_NAM[12]				=	"Names       ";

const uint8_t SX_NUM[12]				=	"Numbers     ";

const uint8_t SX_82[13]					=	"AUDIO msg.  ";

const uint8_t SX_83[13]					=	"SMS msg.    ";

const uint8_t SX_84[13]					=	"Unknown SMS ";

const uint8_t SX_85[13]					=	"Listening-in";

const uint8_t SX_86[13]					=	"List.durat. ";

const uint8_t SX_13x[12]				=	"Exit del.p#";

const uint8_t SX_14x[12]				=	"Warn.del.p#";

const uint8_t SX_15x[12]				=	"Verf.del.p#";

const uint8_t SX_16x[12]				=	"P.# options";

const uint8_t SX_28x[12]				=	"Kpd.# name ";
const uint8_t SX_28xx[11]				=	"Ex.## name";

const uint8_t SX_20[12]					=	"Kpd.address.";
const uint8_t SX_21[12]					=	"Identificat.";


const uint8_t SX_22[12]					=	"Partitions  ";

const uint8_t SX_22x[11]				=	"Kpd.# part.";
const uint8_t SX_22xx[10]				=	"Ex.## part";

const uint8_t txt_strnone[32]			=	"PARTITION       "\
													"NOT SELECTED    ";

const uint8_t txt_qwynone[32]			=	"No output       "\
													"to control      ";

const uint8_t SX_NoAC[12]				=	"Max.AC loss";

const uint8_t SX_23xx[11]				=	"AC.## loss";


const uint8_t SX_24[12]					=	"Chime       ";

const uint8_t SX_24x[12]				=	"Kpd.# chime";


const uint8_t SX_25[12]					=	"Volume      ";

const uint8_t SX_251[11]				=	"Keys       ";
const uint8_t SX_252[11]				=	"Chime      ";
const uint8_t SX_253[11]				=	"Entry delay";
const uint8_t SX_254[11]				=	"Exit delay ";
const uint8_t SX_255[11]				=	"Fire alarm ";
const uint8_t SX_256[11]				=	"Burg.alarm ";
const uint8_t SX_257[11]				=	"Warn.alarm ";
const uint8_t SX_258[11]				=	"New trouble";

const uint8_t SX_251x[11]				=	"Keys #    ";
const uint8_t SX_252x[11]				=	"Chime #   ";
const uint8_t SX_253x[11]				=	"Entry #   ";
const uint8_t SX_254x[11]				=	"Exit #    ";
const uint8_t SX_255x[11]				=	"Fire #    ";
const uint8_t SX_256x[11]				=	"Burg.#    ";
const uint8_t SX_257x[11]				=	"Warn.#    ";
const uint8_t SX_258x[11]				=	"New trbl.#";


const uint8_t SX_26[12]					=	"LCDbacklight";

const uint8_t SX_26x[11]				=	"LCD bl.#   ";


const uint8_t SX_27[12]					=	"KEYbacklight";

const uint8_t SX_27x[11]				=	"KEY bl.#   ";


const uint8_t SX_29[12]					=	"Autolight   ";

const uint8_t SX_29x[11]				=	"Autolight #";


const uint8_t SX_210[11]				=	"ClockFormat";

const uint8_t SX_210x[10]				=	"Clock #   ";


const uint8_t SX_211[11]				=	"Alarms     ";

const uint8_t SX_211x[11]				=	"Alarms #  ";


const uint8_t SX_212x[11]				=	"Kpd.# opts";


const uint8_t SX_218[12]				=	"Connect msg";


const uint8_t SX_31[12]					=	"EOL         ";

const uint8_t SX_31x[12]				=	"Zn.# EOL   ";
const uint8_t SX_31xx[11]				=	"Zn.## EOL ";


const uint8_t SX_32[12]					=	"Sensitivity ";

const uint8_t SX_32x[11]				=	"Zn.# sens. ";
const uint8_t SX_32xx[10]				=	"Zn.## sens";


const uint8_t SX_33[12]					=	"Type        ";

const uint8_t SX_33x[11]				=	"Zn.# type  ";
const uint8_t SX_33xx[10]				=	"Zn.## type";


const uint8_t SX_34[12]					=	"Entry delay ";

const uint8_t SX_34x[11]				=	"Zn.# entry ";
const uint8_t SX_34xx[10]				=	"Z.## entry";


const uint8_t SX_35[12]					=	"Trouble code";

const uint8_t SX_35x[11]				=	"Zn.# trbl. ";
const uint8_t SX_35xx[10]				=	"Z.## trbl.";


const uint8_t SX_361[12]				=	"P.1 zones  ";
const uint8_t SX_362[12]				=	"P.2 zones  ";
const uint8_t SX_363[12]				=	"Night act. ";
const uint8_t SX_364[12]				=	"Day active ";
const uint8_t SX_365[12]				=	"Act.OnePart";
const uint8_t SX_366[12]				=	"Priority   ";
const uint8_t SX_367[12]				=	"3 alarms   ";
const uint8_t SX_368[12]				=	"Bps disable";
const uint8_t SX_369[12]				=	"Shnt.disarm";
const uint8_t SX_370[12]				=	"Viol.event ";
const uint8_t SX_371[12]				=	"Rest.event ";
const uint8_t SX_372[12]				=	"Alarm clear";


const uint8_t SX_39[12]					=	"Arm mode    ";

const uint8_t SX_39x[11]				=	"Zn.# arm   ";
const uint8_t SX_39xx[10]				=	"Zn.## arm ";


const uint8_t SX_41[12]					=	"Function    ";

const uint8_t SX_41x[11]				=	"Function # ";
const uint8_t SX_41xx[10]				=	"Out.## fun";


const uint8_t SX_42[12]					=	"Duration    ";

const uint8_t SX_42x[11]				=	"Out.# dur. ";
const uint8_t SX_42xx[10]				=	"Out.## dur";


const uint8_t SX_43[12]					=	"Zones       ";

const uint8_t SX_43x[12]				=	"Out.# zones";
const uint8_t SX_43xx[11]				=	"O.## zones";


const uint8_t SX_44[12]					=	"Timery      ";

const uint8_t SX_44x[12]				=	"O.# timers ";
const uint8_t SX_44xx[11]				=	"O## timers";


const uint8_t SX_451[12]				=	"P.1 outputs";
const uint8_t SX_452[12]				=	"P.2 outputs";
const uint8_t SX_453[12]				=	"Polarity(+)";
const uint8_t SX_454[12]				=	"Pulsed     ";
const uint8_t SX_455[12]				=	"Arm/Dis/Clr";


const uint8_t SX_46[12]					=	"Quick ctrl. ";


const uint8_t SX_51[12]					=	"Settings    ";

const uint8_t SX_511[11]				=	"Monday     ";
const uint8_t SX_512[11]				=	"Tuesday    ";
const uint8_t SX_513[11]				=	"Wednesday  ";
const uint8_t SX_514[11]				=	"Thursday   ";
const uint8_t SX_515[11]				=	"Friday     ";
const uint8_t SX_516[11]				=	"Saturday   ";
const uint8_t SX_517[11]				=	"Sunday     ";
const uint8_t SX_518[11]				=	"Everyday   ";
const uint8_t SX_5xx[11]				=	"Except.#   ";

const uint8_t SX_53[12]					=	"From        ";

const uint8_t SX_54[12]					=	"Till        ";

const uint8_t SX_59[13]					=	"Active      ";

const uint8_t SX_Str1[12]				=	"Partition 1 ";
const uint8_t SX_Str2[12]				=	"Partition 2 ";

const uint8_t SX_63[13]					=	"Block SIM1  ";
const uint8_t SX_64[13]					=	"Restore SIM1";
const uint8_t SX_65[13]					=	"Block SIM2  ";
const uint8_t SX_66[13]					=	"Restore SIM2";
const uint8_t SX_68[12]					=	"SIM credits ";

const uint8_t SX_681[12]				=	"USSDchkSIM1";
const uint8_t SX_682[12]				=	"USSDchkSIM2";
const uint8_t SX_683[12]				=	"USSDtopSIM1";
const uint8_t SX_684[12]				=	"USSDtopSIM2";
const uint8_t SX_685[12]				=	"Min.cr.SIM1";
const uint8_t SX_686[12]				=	"Min.cr.SIM2";
const uint8_t SX_687[12]				=	"hh:mm SIM1 ";
const uint8_t SX_688[12]				=	"hh:mm SIM2 ";

const uint8_t SX_72[13]					=	"Stations    ";
const uint8_t SX_73[12]					=	"MS1         ";
const uint8_t SX_75[12]					=	"MS2         ";
const uint8_t SX_77[12]					=	"Assign 1    ";
const uint8_t SX_78[12]					=	"Assign 2    ";
const uint8_t SX_79[12]					=	"Test events ";

const uint8_t SX_Ident[12]				=	"Identifiers";
const uint8_t SX_PfSIA[12]				=	"SIA prefix ";
const uint8_t SX_HOWM[12]				=	"Priority   ";
const uint8_t SX_TELAUD[12]			=	"Tel.(AUDIO)";
const uint8_t SX_TELSMS[12]			=	"Tel.(SMS)  ";
const uint8_t SX_ADRIP[11]				=	"Address    ";
const uint8_t SX_PORT[12]				=	"Port       ";
const uint8_t SX_FORMAT[12]			=	"Format     ";
const uint8_t SX_KlSTAM[12]			=	"STAM key   ";
const uint8_t SX_KlGPRS[12]			=	"GPRS key   ";
const uint8_t SX_FmtSMS[12]			=	"SMS format ";
const uint8_t SX_acct[12]				=	"SIA-IP acct";
const uint8_t SX_Ksiaip[12]			=	"SIA-IP key ";
const uint8_t SX_Osiaip[12]			=	"SIA-IP test";

const uint8_t SX_7x1[11]				=	"Zones      ";
const uint8_t SX_7x2[11]				=	"Partitions ";
const uint8_t SX_7x3[11]				=	"Expanders  ";
const uint8_t SX_7x4[12]				=	"Syst.events";
const uint8_t SX_7x5[12]				=	"Syst.rest. ";
const uint8_t SX_7x6[12]				=	"Others     ";

const uint8_t SX_7x11[11]				=	"Alarm     ";
const uint8_t SX_7x12[11]				=	"Al.restore";
const uint8_t SX_7x13[11]				=	"Tamper    ";
const uint8_t SX_7x14[11]				=	"Tamp.rest.";
const uint8_t SX_7x15[11]				=	"Bypass    ";
const uint8_t SX_7x16[11]				=	"Unbypass  ";
const uint8_t SX_7x17[11]				=	"Trouble   ";
const uint8_t SX_7x18[11]				=	"Trbl.rest.";

const uint8_t SX_7x21[11]				=	"Arm       ";
const uint8_t SX_7x22[11]				=	"Disarm    ";
const uint8_t SX_7x23[11]				=	"Al.clear  ";
const uint8_t SX_7x24[11]				=	"Arm fail. ";
const uint8_t SX_7x25[11]				=	"Kfb.panic ";
const uint8_t SX_7x26[11]				=	"Kfb.medic.";
const uint8_t SX_7x27[11]				=	"Kfb.fire  ";

const uint8_t SX_7x31[11]				=	"Restarts  ";
const uint8_t SX_7x32[11]				=	"Duress    ";
const uint8_t SX_7x33[11]				=	"Panic     ";
const uint8_t SX_7x34[11]				=	"Medical   ";
const uint8_t SX_7x35[11]				=	"Fire      ";
const uint8_t SX_7x36[11]				=	"Tamper    ";
const uint8_t SX_7x37[11]				=	"Tamp.rest.";
const uint8_t SX_7x38[11]				=	"3wrng.code";
const uint8_t SX_7x39[11]				=	"AC trouble";
const uint8_t SX_7x40[11]				=	"AC restore";
const uint8_t SX_7x41[11]				=	"BAT miss. ";
const uint8_t SX_7x42[11]				=	"BATm.rest.";
const uint8_t SX_7x43[11]				=	"BAT low   ";
const uint8_t SX_7x44[11]				=	"BATl.rest.";

const uint8_t SX_791[12]				=	"At         ";
const uint8_t SX_792[12]				=	"Disarmed   ";
const uint8_t SX_793[12]				=	"Armed      ";

const uint8_t SX_95[12]					=	"Troubles    ";
const uint8_t SX_96[12]					=	"Outputs     ";

const uint8_t SX_9x1[11]				=	"Arm        ";
const uint8_t SX_9x2[11]				=	"Disarm     ";
const uint8_t SX_9x3[11]				=	"Alarm clear";
const uint8_t SX_9x4[11]				=	"Arm fail.  ";
const uint8_t SX_9x5[11]				=	"Alarm      ";
const uint8_t SX_9x6[11]				=	"Tamper     ";
const uint8_t SX_9x7[11]				=	"Tamp.rest. ";
const uint8_t SX_9x8[11]				=	"Panic      ";
const uint8_t SX_9x9[11]				=	"Medical    ";
const uint8_t SX_9x10[10]				=	"Fire      ";
const uint8_t SX_9x11[10]				=	"Duress    ";

const uint8_t SX_951[11]				=	"BAT low    ";
const uint8_t SX_952[11]				=	"BATl.rest. ";
const uint8_t SX_953[11]				=	"AC trbl.   ";
const uint8_t SX_954[11]				=	"AC rest.   ";
const uint8_t SX_955[11]				=	"GSM tr.rest";

const uint8_t SX_111[12]				=	"USSD SIM1  ";
const uint8_t SX_112[12]				=	"USSD SIM2  ";
const uint8_t SX_113[12]				=	"Chk.credit1";
const uint8_t SX_114[12]				=	"Chk.credit2";
const uint8_t SX_115[12]				=	"PERF.Soft  ";
const uint8_t SX_116[12]				=	"Download FW";
const uint8_t SX_117[12]				=	"Update FW  ";
const uint8_t SX_118[12]				=	"SMS control";
const uint8_t SX_119[12]				=	"SMS funct. ";
const uint8_t SX_1110[12]				=	"Any number ";
const uint8_t SX_1111[11]				=	"FW d-loaded";
const uint8_t SX_1112[11]				=	"FW notfound";
const uint8_t SX_1113[11]				=	"FW error   ";
const uint8_t SX_1114[11]				=	"FW updated ";
const uint8_t SX_1115[11]				=	"FW not upd.";

const uint8_t SX_118x[11]				=	"SMS #     ";
const uint8_t SX_118xx[10]				=	"SMS ##   ";

const uint8_t SX_119x[11]				=	"Funct.#   ";
const uint8_t SX_119xx[10]				=	"Funct.## ";

const uint8_t SX_121[11]				=	"Schedules  ";

const uint8_t SX_121x[11]				=	"Schedule #";

const uint8_t SX_121n[11]				=	"Sch.# name";

const uint8_t SX_122[11]				=	"Kfb.funct. ";
const uint8_t SX_124[12]				=	"Al.duration";
const uint8_t SX_125[12]				=	"Suppr.arm  ";
const uint8_t SX_127[11]				=	"Radio devs ";

const uint8_t SX_1271[10]				=	"Add       ";
const uint8_t SX_1272[11]				=	"Filter    ";
const uint8_t SX_1273[10]				=	"Remove    ";
const uint8_t SX_1274[10]				=	"Out.tamper";
const uint8_t SX_1275[11]				=	"Al.signal.";
const uint8_t SX_1276[11]				=	"Acknowled.";

const uint8_t txt_1271_a[15]			=	"Serial number  ";

const uint8_t txt_1271_b[24]			=	"Open tamper     "\
													"device  ";

const uint8_t txt_100_supp[14]		=	"Function ##   ";

const uint8_t txt_7x4[15*16]			=	"PERF-Soft conn. "\
													"SM start        "\
													"AC trouble      "\
													"BAT missing     "\
													"BAT low         "\
													"MS1 trouble     "\
													"MS2 trouble     "\
													"RTC setting     "\
													"OUT1 trouble    "\
													"OUT2 trouble    "\
													"AUX trouble     "\
													"KPD trouble     "\
													"DTA trouble     "\
													"GSM trouble     "\
													"Radio jamming   ";

const uint8_t txt_7x5[15*16]			=	"PERF-Soft disc. "\
													"SM end          "\
													"AC restore      "\
													"BAT miss.rest.  "\
													"BAT low restore "\
													"MS1 restore     "\
													"MS2 restore     "\
													"RTC trouble     "\
													"OUT1 restore    "\
													"OUT2 restore    "\
													"AUX restore     "\
													"KPD restore     "\
													"DTA restore     "\
													"GSM restore     "\
													"Radio jam.rest. ";

const uint8_t txt_7x6[4*16]			=	"PERFECTA restart"\
													"RAM error       "\
													"Manul test      "\
													"Period test     ";


const uint8_t txt_061[5*16]			=	"No time change  "\
													"UE standard     "\
													"US standard     "\
													"1h by dates     "\
													"2h by dates     ";


const uint8_t txt_26x[6*16]			=	"    no backlight"\
													"             50%"\
													"            100%"\
													"      auto 0-50%"\
													"     auto 0-100%"\
													"    auto 50-100%";


const uint8_t txt_27x[3*16]			=	"    no backlight"\
													"            auto"\
													"       permanent";


const uint8_t txt_29_none[32]			=	"No              "\
													"auto backlight  ";
const uint8_t txt_29_we[32]			=	"Zn.## violation:";
const uint8_t txt_29_str[32]			=	"P.# entry delay:";


const uint8_t txt_210x[8*16]			=	"           hh:mm"\
													"        hh:mm:ss"\
													"dd mmm yy, hh:mm"\
													"dd mmm, hh:mm:ss"\
													" yy-mm-dd, hh:mm"\
													"yyyy-mm-dd hh:mm"\
													"DOW dd mmm,hh:mm"\
													"keypad name     ";


const uint8_t txt_211x[5*16]			=	"3 wrng codes al."\
													"Medical alarm   "\
													"Fire alarm      "\
													"Panic alarm     "\
													"Silent panic    ";


const uint8_t txt_212x[10*16]			=	"Show part.1     "\
													"Show part.2     "\
													"Quickarm part.1 "\
													"Quickarm part.2 "\
													"Show code enter."\
													"Quick control   "\
													"Troubles review "\
													"Chime on/off    "\
													"Disp.mode change"\
													"Wake up         ";


const uint8_t txt_121x[12*16]			=	"Arm             "\
													"Disarm          "\
													"Alarm clear     "\
													"Duress          "\
													"Zones inhibit   "\
													"Zones isolate   "\
													"Code change     "\
													"Users edit      "\
													"Outputs control "\
													"Tests           "\
													"Service access  "\
													"ID change       ";


const uint8_t txt_126[16*16]			=	"Grade2          "\
													"Troubles memory "\
													"3wrng.codes=blk."\
													"No AC=no bcklght"\
													"Restore events  "\
													"Events limitat. "\
													"Tmp.on ext.siren"\
													"Tmp.on int.siren"\
													"Trbl.in part.arm"\
													"No SATEL trouble"\
													"No jamm. trouble"\
													"Usr.replaces BAT"\
													"Check if ready  "\
													"Arm ExDly w.trbl"\
													"Tamper = no arm "\
													"BAT low = no arm";


const uint8_t SX_CENT[12]				=	"SMS centre ";


const uint8_t txt_100[2*16]			=	"SMS messaging   "\
													"Messaging events";


const uint8_t txt_eol_brak[16]		=	"0.Not used      ";
const uint8_t txt_eol_nc[16]			=	"1.EOL=0 (NC)    ";
const uint8_t txt_eol_no[16]			=	"2.EOL=0 (NO)    ";
const uint8_t txt_eol_eol[16]			=	"3.EOL=1         ";
const uint8_t txt_eol_2eolnc[16]		=	"4.EOL=2 (NC)    ";
const uint8_t txt_eol_2eolno[16]		=	"5.EOL=2 (NO)    ";
const uint8_t txt_eol_rolnc[16]		=	"6.Roller        ";
const uint8_t txt_eol_wibnc[16]		=	"7.Vibration     ";
;/// const uint8_t txt_eol_analog[16]		=	"8.Analog        ";


const uint8_t txt_fn_wewy[16]			=	"0.Entry/Exit    ";
const uint8_t txt_fn_wewy_fin[16]	=	"1.En/Ex final   ";
const uint8_t txt_fn_wewn[16]			=	"2.En/Ex route   ";
const uint8_t txt_fn_natych[16]		=	"3.Instant       ";
const uint8_t txt_fn_dwukrotna[16]	=	"4.Double knock  ";
const uint8_t txt_fn_24h_wlam[16]	=	"5.24h burglary  ";
const uint8_t txt_fn_24h_sabot[16]	=	"6.24h tamper    ";
const uint8_t txt_fn_24h_napad[16]	=	"7.24h panic     ";
const uint8_t txt_fn_24h_cicha[16]	=	"8.24h sil.panic ";
const uint8_t txt_fn_24h_pomoc[16]	=	"9.24h medical   ";
const uint8_t txt_fn_24h_pozar[16]	=	"10.24h fire     ";
const uint8_t txt_fn_24h_mask[16]	=	"11.Mask.detector";
const uint8_t txt_fn_nieuzywana[16]	=	"12.No alarm act.";
const uint8_t txt_fn_zalwyl[16]		=	"13.Arm/Disarm   ";
const uint8_t txt_fn_zal[16]			=	"14.Arm          ";
const uint8_t txt_fn_wyl[16]			=	"15.Disarm       ";
const uint8_t txt_fn_koncz_Twy[16]	=	"16.Ex.del.term. ";
const uint8_t txt_fn_czuj_rygla[16]	=	"17.Shunt lock   ";
const uint8_t txt_fn_odbl_opozn[16]	=	"18.En.rout.enbl.";
const uint8_t txt_fn_awaria[16]		=	"19.Trouble      ";


const uint8_t txt_yf_nieuzywane[16]	=	"0.Not used      ";
const uint8_t txt_yf_sygzew[16]		=	"1.External siren";
const uint8_t txt_yf_sygwew[16]		=	"2.Internal siren";
const uint8_t txt_yf_alwlam[16]		=	"3.Burglary alarm";
const uint8_t txt_yf_alpozar[16]		=	"4.Fire alarm    ";
const uint8_t txt_yf_alprzym[16]		=	"5.Duress alarm  ";
const uint8_t txt_yf_alnapad[16]		=	"6.Panic alarm   ";
const uint8_t txt_yf_alpomoc[16]		=	"7.Medical alarm ";
const uint8_t txt_yf_alniezwer[16]	=	"8.Unverified al.";
const uint8_t txt_yf_alzwer[16]		=	"9.Verified alarm";
const uint8_t txt_yf_alsabot[16]		=	"10.Tamper alarm ";
const uint8_t txt_yf_zaspozar[16]	=	"11.Supply fire  ";
const uint8_t txt_yf_zasczuw[16]		=	"12.Supply armed ";
const uint8_t txt_yf_narwej[16]		=	"13.Zone violat. ";
const uint8_t txt_yf_gong[16]			=	"14.Chime        ";
const uint8_t txt_yf_sterowalne[16]	=	"15.Control      ";
const uint8_t txt_yf_gotowy[16]		=	"16.READY status ";
const uint8_t txt_yf_Twy[16]			=	"17.Exit delay s.";
const uint8_t txt_yf_czuw[16]			=	"18.Armed status ";
const uint8_t txt_yf_awarii[16]		=	"19.Trouble stat.";
const uint8_t txt_yf_alczu[16]		=	"20.Al/Arm status";
const uint8_t txt_yf_czuj[16]			=	"21.Zones reset  ";
const uint8_t txt_yf_TS[16]			=	"22.SM status    ";
const uint8_t txt_yf_czuwmon[16]		=	"23.Arm stat.mon.";


const uint8_t txt_cod_brak[12]		=	"Not monitor.";
const uint8_t txt_cod_151[12]			=	"Gaz detected";
const uint8_t txt_cod_152[12]			=	"Refrigerat. ";
const uint8_t txt_cod_153[12]			=	"Heat loss   ";
const uint8_t txt_cod_154[12]			=	"H2O leakage ";
const uint8_t txt_cod_155[12]			=	"Foil break  ";
const uint8_t txt_cod_156[12]			=	"Day trouble ";
const uint8_t txt_cod_157[12]			=	"Low gas lvl.";
const uint8_t txt_cod_158[12]			=	"High temp.  ";
const uint8_t txt_cod_159[12]			=	"Low temp.   ";
const uint8_t txt_cod_161[12]			=	"Airflow low ";
const uint8_t txt_cod_162[12]			=	"CO detected ";
const uint8_t txt_cod_163[12]			=	"Tank level  ";
const uint8_t txt_cod_201[12]			=	"H2O prss.low";
const uint8_t txt_cod_202[12]			=	"CO2 prss.low";
const uint8_t txt_cod_203[12]			=	"Gate valve  ";
const uint8_t txt_cod_204[12]			=	"H2O levl.low";
const uint8_t txt_cod_205[12]			=	"Pump activ. ";
const uint8_t txt_cod_206[12]			=	"Pump failure";


const uint8_t txt_czuw_0123[4*16]	=	"No Arm/Disarm   "\
													"Arm (full)      "\
													"Arm (night)     "\
													"Arm (day)       ";


const uint8_t txt_03[2*16]				=	"SM sounds       "\
													"Block SM        ";


const uint8_t txt_16x[2*16]			=	"Infinit.ex.delay"\
													"Fin.exit delay  ";


const uint8_t txt_67[7*16]				=	"PERFECTA Soft   "\
													"PERFECTA CONTROL"\
													"PUSH messages   "\
													"GSM network time"\
													"NTP server time "\
													"USSD any tel.   "\
													"FW adr.from SMS ";


const uint8_t txt_o7x5[7*16]			=	"UDP             "\
													"SIA-IP          "\
													"Names in SIA    "\
													"National chars  "\
													"Timestamp SIA-IP"\
													"SIA-IP encrypt. "\
													"SIA prefix      ";


const uint8_t txt_o794[16]				=	"Independ.test   ";


const uint8_t SX_Tzaw[12]				=	"Suspen.time";

const uint8_t txt_wait[32]				=	"Please wait...  "\
													"                ";

const uint8_t txt_experr[32]			=	"Expander 0x##   "\
													"trouble         ";

const uint8_t txt_expfnd[32]			=	"Found: #        "\
													"                ";

const uint8_t txt_factory[32]			=	"Factory         "\
													"settings ? 1=Yes";

const uint8_t txt_name_serv[16]		=	"Service         ";

const uint8_t txt_name_user[16]		=	"User ##         ";

const Ttxt_14_2 txt_name_str = {			"Partition #   ",
	32,32
};

const struct {
	const uint8_t filling1[15];
	const uint8_t filling2[1];
} txt_name_exp = {							"Expander   0x##",
	32
};


const uint8_t txt_shrt_wej[11]		=	"Zone  #   ";

const Ttxt_10_6 txt_name_wej = {			"Zone ##   ",
	{32,32,32,32,32,32}
};


const uint8_t txt_shrt_wyj[11]		=	"Output  # ";

const Ttxt_10_6 txt_name_wyj = {			"Output ## ",
	{32,32,32,32,32,32}
};


const struct {
	const uint8_t filling1[11];
	const uint8_t filling2[5];
} txt_name_tel = {							"Phone #    ",
	{32,32,32,32,32}
};

const struct {
	const uint8_t filling1[10];
	const uint8_t filling2[6];
} txt_name_tim = {							"Timer #   ",
	{32,32,32,32,32,32}
};

const uint8_t txt_name_sch[5*16]		=	"Normal          "\
													"Simple          "\
													"Arms only       "\
													"Duress          "\
													"Master          ";

const uint8_t txt_invit_msg[16]		=	"Connecting...   ";

const uint8_t txt_sms_fw_get[32]		=	"Firmware downloaded             ";
const uint8_t txt_sms_fw_nonew[32]	=	"No newer firmware               ";
const uint8_t txt_sms_fw_err[32]		=	"Error downloading firmware      ";
const uint8_t txt_sms_fw_lack[32]	=	"Firmware not yet downloaded     ";
const uint8_t txt_sms_fw_ok[32]		=	"Firmware updated                ";

const uint8_t txt_72[4*16]				=	"MS1 or MS2      "\
													"MS1             "\
													"MS2             "\
													"MS1 and MS2     ";

const uint8_t txt_cid_all[16]			=	"CID all         ";
const uint8_t txt_cid_sel[16]			=	"CID selected    ";
const uint8_t txt_sia_all[16]			=	"SIA all         ";
const uint8_t txt_sia_sel[16]			=	"SIA selected    ";

const uint8_t txt_typzdarzen[15]		=	"Events type    ";

const uint8_t txt_typzd_1[16]			=	"Alarm           ";
const uint8_t txt_typzd_2[16]			=	"Arm/Disarm/Clear";
const uint8_t txt_typzd_3[16]			=	"Bypass          ";
const uint8_t txt_typzd_5[16]			=	"Troubles        ";
const uint8_t txt_typzd_6[16]			=	"Function        ";
const uint8_t txt_typzd_7[16]			=	"System          ";

const uint8_t txt_radsyg_s[16]		=	"Sound#          ";
const uint8_t txt_radsyg_o[16]		=	"Light           ";
const uint8_t txt_radsyg_os[16]		=	"Light + sound#  ";


const struct {
	const uint8_t filling1[12];
	const uint8_t filling2[4];
} txt_Twe = {									"entry delay:",
	{35,35,35,Spec_sec}
};


const struct {
	const uint8_t filling1[12];
	const uint8_t filling2[4];
} txt_Twy = {									"exit delay: ",
	{35,35,35,Spec_sec}
};


const struct {
	const uint8_t filling1[12];
	const uint8_t filling2[4];
} txt_WRN = {									"warn.delay: ",
	{35,35,35,Spec_sec}
};


const struct {
	const uint8_t filling1[12];
	const uint8_t filling2[4];
} txt_VRF = {									"verif.delay:",
	{35,35,35,Spec_min}
};


const struct {
	const uint8_t filling1[4];
	const uint8_t filling2[12];
} txt_tim_pon = {								"Mon:",
	{32,35,35,58,35,35,32,35,35,58,35,35}
};


const struct {
	const uint8_t filling1[4];
	const uint8_t filling2[12];
} txt_tim_wto = {								"Tue:",
	{32,35,35,58,35,35,32,35,35,58,35,35}
};


const struct {
	const uint8_t filling1[4];
	const uint8_t filling2[12];
} txt_tim_sro = {								"Wed:",
	{32,35,35,58,35,35,32,35,35,58,35,35}
};


const struct {
	const uint8_t filling1[4];
	const uint8_t filling2[12];
} txt_tim_czw = {								"Thu:",
	{32,35,35,58,35,35,32,35,35,58,35,35}
};


const struct {
	const uint8_t filling1[4];
	const uint8_t filling2[12];
} txt_tim_pia = {								"Fri:",
	{32,35,35,58,35,35,32,35,35,58,35,35}
};


const struct {
	const uint8_t filling1[4];
	const uint8_t filling2[12];
} txt_tim_sob = {								"Sat:",
	{32,35,35,58,35,35,32,35,35,58,35,35}
};


const struct {
	const uint8_t filling1[4];
	const uint8_t filling2[12];
} txt_tim_nie = {								"Sun:",
	{32,35,35,58,35,35,32,35,35,58,35,35}
};


const struct {
	const uint8_t filling1[4];
	const uint8_t filling2[12];
} txt_tim_cod = {								"Evd:",
	{32,35,35,58,35,35,32,35,35,58,35,35}
};


const struct {
	const uint8_t filling1[4];
	const uint8_t filling2[12];
} txt_tim_wy1 = {								"Ex1:",
	{32,35,35,58,35,35,32,35,35,58,35,35}
};


const struct {
	const uint8_t filling1[4];
	const uint8_t filling2[12];
} txt_tim_wy2 = {								"Ex2:",
	{32,35,35,58,35,35,32,35,35,58,35,35}
};


const struct {
	const uint8_t filling1[4];
	const uint8_t filling2[12];
} txt_tim_wy3 = {								"Ex3:",
	{32,35,35,58,35,35,32,35,35,58,35,35}
};


const struct {
	const uint8_t filling1[4];
	const uint8_t filling2[12];
} txt_tim_wy4 = {								"Ex4:",
	{32,35,35,58,35,35,32,35,35,58,35,35}
};


const struct {
	const uint8_t filling1[6];
	const uint8_t filling2[10];
} txt_tim_od = {								"from: ",
	{35,35,35,35,45,35,35,45,35,35}
};


const struct {
	const uint8_t filling1[6];
	const uint8_t filling2[10];
} txt_tim_do = {								"till: ",
	{35,35,35,35,45,35,35,45,35,35}
};
