Spec_month.b	equ 'm'		; char to indicate months
Spec_day.b	equ 'd'		; char to indicate days
Spec_hour.b	equ 'h'		; char to indicate hours
Spec_min.b	equ 'm'		; char to indicate minutes
Spec_sec.b	equ 's'		; char to indicate seconds
Spec_volt.b	equ 'V'		; char to indicate Volt (voltage)

Spec_red.b	equ 'R'		; char to indicate RED color
Spec_green.b	equ 'G'		; char to indicate GREEN color
Spec_yellow.b	equ 'Y'		; char to indicate YELLOW color

Trbls_mem_char.b	equ 'M'		; char to indicate trouble memory

WE_LED_bypass.b		equ 'b'		; char to indicate zone bypass
WE_LED_long.b		equ 'L'		; char to indicate zone long violation trouble
WE_LED_lack.b		equ 'N'		; char to indicate zone no violation trouble
WE_LED_1st.b		equ '!'		; char to indicate 1st alarming zone
;(**) WE_LED_TampAl.b	equ 'T'		; char to indicate zone tamper alarm
;(**) WE_LED_Alarm.b	equ 'A'		; char to indicate zone alarm
WE_LED_Tamper.b		equ Spec_box	; char to indicate zone tamper
WE_LED_Viol.b		equ Spec_ball	; char to indicate zone violation
WE_LED_TampMem.b	equ 't'		; char to indicate zone tamper alarm memory
WE_LED_AlMem.b		equ 'a'		; char to indicate zone alarm memory
WE_LED_ok.b		equ Spec_dot	; char to indicate zone is ok


		dc.t 0
MU_funmenu:	; menu - code change
		dc.b "Change code  "
		dc.t Is_code
		dc.t {0100000h+Go_code}
MU_user_mn:	; menu - users
		dc.b "Users        "
		dc.t Is_users
		dc.t {0280000h+MU_users}
		; menu - abort voice messaging
		dc.b "Abort v.msg. "
		dc.t Is_abortVM
		dc.t {0300000h+Go_abortVM}
MU_bps_mn:	; menu - bypasses
		dc.b "Bypasses     "
		dc.t Is_bypass
		dc.t {0480000h+MU_bypass}
MU_ev_mn:	; menu - view events log
		dc.b "Event log    "
		dc.t Is_events
		dc.t {0500000h+Go_events}
MU_sett_mn:	; menu - settings
		dc.b "Settings     "
		dc.t Is_sets
		dc.t {0680000h+MU_settings}
		; menu - view troubles
		dc.b "System state "
		dc.t IS_7
		dc.t {0700000h+UF_7}
		; menu - output control
		dc.b "Control      "
		dc.t Is_ctrl
		dc.t {0800000h+Go_ctrl}
MU_test_mn:	; menu - tests
		dc.b "Tests        "
		dc.t Is_tests
		dc.t {0980000h+MU_tests}
MU_serv_mn:	; menu - service and download
		dc.b "Service      "
		dc.t Is_sermenu
		dc.t {0080000h+MU_servmenu}
		; menu - end of menu
		dc.b 0
		dc.t 0


		dc.t 0
MU_events:	; menu - All events
		dc.b "All          "
		dc.t Is_always
		dc.t {0100000h+Go_ev_all}
		; menu - Backup events
		dc.b "Grade2 backup"
		dc.t Is_always
		dc.t {0200000h+Go_ev_backup}
		; menu - end of menu
		dc.b 0
		dc.t MU_ev_mn


		dc.t 0
MU_servmenu:	; menu - Service Mode
		dc.b "Service Mode "
		dc.t Is_UF_00
		dc.t {0000000h+Go_Service}
		; menu - Start DWNL-TEL
		dc.b "Start DwnlTEL"
		dc.t Is_DX_tel
		dc.t {0100000h+Go_DX_tel}
 #if {{typ_centrali lt 5} and {VeIP eq 0}}
MU_gsmac:	; menu - Start DWNL-GSM
		dc.b "Start DwnlGSM"
		dc.t Is_DX_gsm
		dc.t {0280000h+MU_DXGSM}
 #endif
		; menu - Start DWNL-RS
 #if {typ_centrali lt 5}
		dc.b "Start DwnlUSB"
 #else
		dc.b "Start DwnlRS "
 #endif
		dc.t Is_DWNLRSon
		dc.t {0300000h+Go_DWNLRSon}
		; menu - Finish DWNL-RS
 #if {typ_centrali lt 5}
		dc.b "FinishDwnlUSB"
 #else
		dc.b "Finish DwnlRS"
 #endif
		dc.t Is_DWNLRSoff
		dc.t {0400000h+Go_DWNLRSoff}
		; menu - Service permanent access
		dc.b "Serv.access "
		dc.b 32
		dc.t Is_not_serv
		dc.t {0500000h+Go_SeAcPerm}
		; menu - Service access time
		dc.b "Access time  "
		dc.t Is_SeAcTime
		dc.t {0600000h+Go_SeAcTime}
		; menu - Start DWNL-ETHM-1
		dc.b 69,84,72,77,45,49,Arr_right,68,76,79,65,68,88
		dc.t Is_ETHMon
		dc.t {0700000h+Go_ETHMon}
 #if {{typ_centrali lt 5} and {VeIP eq 0}}
		; menu - Start DWNL-GPRS
		dc.b 71,80,82,83,Arr_right,68,76,79,65,68,88,32,32
		dc.t Is_GPRSon
		dc.t {0800000h+Go_GPRSon}
 #endif
		; menu - end of menu
		dc.b 0
		dc.t MU_serv_mn


 #if {{typ_centrali lt 5} and {VeIP eq 0}}
		dc.t 0
MU_DXGSM:	; menu - DWNL GSM audio
		dc.b "GSM audio    "
		dc.t Is_DX_gsm
		dc.t {0100000h+Go_DX_gsm}
		; menu - DWNL GSM CSD
		dc.b "GSM CSD      "
		dc.t Is_DX_gsm
		dc.t {0200000h+Go_DX_csd}
		; menu - end of menu
		dc.b 0
		dc.t MU_gsmac
 #endif


		dc.t 0
MU_settings:	; menu - Autoarm defer
		dc.b "A-arm defer. "
		dc.t Is_def
		dc.t {0100000h+Go_def}
		; menu - RTC setting
		dc.b "RTC clock    "
		dc.t Is_RTC
		dc.t {0200000h+Go_RTC}
		; menu - timer setting
		dc.b "Timers       "
		dc.t Is_timer
		dc.t {0300000h+Go_timer}
		; menu - tel. setting
		dc.b "Tel. numbers "
		dc.t Is_nrtel
		dc.t {0400000h+Go_nrtel}
		; menu - messaging clearing codes setting
		dc.b "Msg.clr.codes"
		dc.t Is_nrkas
		dc.t {0500000h+Go_pwdcds}
		; menu - end of menu
		dc.b 0
		dc.t MU_sett_mn


		dc.t 0
MU_users:	; menu - new user
		dc.b "New user     "
		dc.t Is_nwusr
		dc.t {0100000h+Go_nwusr}
		; menu - edit user
		dc.b "Edit user    "
		dc.t Is_edusr
		dc.t {0200000h+Go_edusr}
		; menu - remove user
		dc.b "Remove user  "
		dc.t Is_rmusr
		dc.t {0300000h+Go_rmusr}
		; menu - end of menu
		dc.b 0
		dc.t MU_user_mn


		dc.t 0
MU_bypass:	; menu - inhibit
		dc.b "Inhibit      "
		dc.t Is_inhibit
		dc.t {0100000h+Go_inhibit}
		; menu - isolate
		dc.b "Isolate      "
		dc.t Is_isolate
		dc.t {0200000h+Go_isolate}
		; menu - end of menu
		dc.b 0
		dc.t MU_bps_mn


		dc.t 0
MU_tests:	; menu - zone test
		dc.b "Zone test    "
		dc.t Is_always
		dc.t {0100000h+Go_tst_we}
		; menu - output test
		dc.b "Output test  "
		dc.t Is_always
		dc.t {0200000h+Go_tst_wy}
 #if {{typ_centrali lt 5} and {VeIP eq 0}}
		; menu - ABAX devices / GSM signal level
		dc.b "Wrls/GSM sig."
 #else
		; menu - ABAX devices signal level
		dc.b "Wireless sig."
 #endif
		dc.t Fis_tst_abax
		dc.t {0300000h+Go_tst_abax}
		; menu - manual monitoring test
		dc.b "Manual MS tst"
		dc.t Fis_tst_trtst
		dc.t {0400000h+Go_tst_trtst}
		; menu - monitoring station 1 test
		dc.b "MS1 test     "
		dc.t Fis_tst_trsm1
		dc.t {0500000h+Go_tst_trsm1}
		; menu - monitoring station 2 test
		dc.b "MS2 test     "
		dc.t Fis_tst_trsm2
		dc.t {0600000h+Go_tst_trsm2}
		; menu - VERSA version
		dc.b "VERSA version"
		dc.t Fis_tst_verV
		dc.t {0700000h+kpd_INFO}
		; menu - expander version
		dc.b "Expander ver."
		dc.t Fis_tst_verE
		dc.t {0800000h+Go_tst_verE}
		; menu - outputs reset
		dc.b "Supply volt. "
		dc.t Fis_tst_volt
		dc.t {0900000h+Go_tst_volt}
		; menu - outputs reset
		dc.b "Outputs reset"
		dc.t Fis_tst_rstWY
		dc.t {0000000h+Go_tst_rstWY}
		; menu - end of menu
		dc.b 0
		dc.t MU_test_mn


		dc.t 0
SRV_mainmenu:
SRV_0_bs:	; service - SM configuration
		dc.b "SrvMod config"
		dc.t {0080000h+SRV_0_menu}
SRV_1_bs:	; service - Partitions
		dc.b "Partitions   "
		dc.t {0180000h+SRV_1_menu}
SRV_2_bs:	; service - Hardware
		dc.b "Hardware     "
		dc.t {0280000h+SRV_2_menu}
SRV_3_bs:	; service - Options
		dc.b "Global param."
		dc.t {0380000h+SRV_3_menu}
SRV_4_bs:	; service - Timers
		dc.b "Timers       "
		dc.t {0480000h+SRV_4_menu}
SRV_5_bs:	; service - Monitoring
		dc.b "Monitoring   "
		dc.t {0580000h+SRV_5_menu}
SRV_6_bs:	; service - Messaging
		dc.b "Messaging    "
		dc.t {0680000h+SRV_6_menu}
SRV_7_bs:	; service - Answering
		dc.b "Answering    "
		dc.t {0780000h+SRV_7_menu}
SRV_8_bs:	; service - Users templates
		dc.b "Usr templates"
		dc.t {0880000h+SRV_8_menu}
SRV_9_bs:	; service - User menu
		dc.b "User menu    "
		dc.t {0900000h+SF_9}
		; service - end of menu
		dc.b 0
		dc.t 0


		dc.t 0
SRV_0_menu:	; service - End service
		dc.b "Quit SrvMod  "
		dc.t {0000000h+SF_00}
		; service - VERSA ident.
		dc.b "VERSA id.    "
		dc.t {0100000h+SF_01}
		; service - DLOADX1 ident.
		dc.b "DLOADX id.   "
		dc.t {0200000h+SF_02}
		; service - DLOADX2 ident.
		;dc.b "DLOADX2 id.  "
		;dc.t {0300000h+SF_03}
		; service - DLOADX1 tel. No
		dc.b "DLOADX tel.  "
		dc.t {0400000h+SF_04}
 #if {{typ_centrali lt 5} and {VeIP eq 0}}
		; service - DLOADX2 tel. No
		dc.b "DLOADX GSM   "
		dc.t {0500000h+SF_05}
 #endif
		; service - SM options
		dc.b "SrvMod opt. "
		dc.b 32
		dc.t {0600000h+SF_06}
		; service - Restore all
		dc.b "Restore all  "
		dc.t {0700000h+SF_07}
		; service - Restore users
		dc.b "Default usr. "
		dc.t {0800000h+SF_08}
 #if {typ_centrali ne 4}
		; service - STARTER
		dc.b "STARTER      "
		dc.t {0900000h+SF_09}
 #endif
		; service - Hide service
		dc.b "Hide SM now  "
		dc.t {0A00000h+SF_0A}
		; service - end of menu
		dc.b 0
		dc.t SRV_0_bs


		dc.t 0
SRV_1_menu:	; service - Partition 1 zones
		dc.b "Part.1 zones"
		dc.b 32
		dc.t {0100000h+SF_11}
		; service - Partition 2 zones
		dc.b "Part.2 zones"
		dc.b 32
		dc.t {0200000h+SF_12}
SRV_13_bs:	; service - Partition 1 times
		dc.b "Part.1 times "
		dc.t {0380000h+SRV_13_menu}
SRV_14_bs:	; service - Partition 2 times
		dc.b "Part.2 times "
		dc.t {0480000h+SRV_14_menu}
		; service - Partition 1 name
		dc.b "Part.1 name  "
		dc.t {0500000h+SF_15}
		; service - Partition 2 name
		dc.b "Part.2 name  "
		dc.t {0600000h+SF_16}
		; service - Partition options
		dc.b "Part. options"
		dc.t {0700000h+SF_17}
		; service - end of menu
		dc.b 0
		dc.t SRV_1_bs


		dc.t 0
SRV_13_menu:	; service - exit time
		dc.b "Exit delay   "
		dc.t {0100000h+SF_131}
		; service - entry time
		dc.b "Entry delay  "
		dc.t {0200000h+SF_132}
		; service - warning time
		dc.b "Warning      "
		dc.t {0300000h+SF_133}
		; service - alarm verification time
		dc.b "Verification "
		dc.t {0400000h+SF_134}
		; service - autoarm delay
		dc.b "Autoarm delay"
		dc.t {0500000h+SF_135}
		; service - autoarm time extension
		dc.b "A-arm defer. "
		dc.t {0600000h+SF_136}
		; service - end of menu
		dc.b 0
		dc.t SRV_13_bs


		dc.t 0
SRV_14_menu:	; service - exit time
		dc.b "Exit delay   "
		dc.t {0100000h+SF_141}
		; service - entry time
		dc.b "Entry delay  "
		dc.t {0200000h+SF_142}
		; service - warning time
		dc.b "Warning      "
		dc.t {0300000h+SF_143}
		; service - alarm verification time
		dc.b "Verification "
		dc.t {0400000h+SF_144}
		; service - autoarm delay
		dc.b "Autoarm delay"
		dc.t {0500000h+SF_145}
		; service - autoarm time extension
		dc.b "A-arm defer. "
		dc.t {0600000h+SF_146}
		; service - end of menu
		dc.b 0
		dc.t SRV_14_bs


		dc.t 0
SRV_2_menu:
SRV_21_bs:	; service - expanders
		dc.b "Kpds. & exps."
		dc.t {0180000h+SRV_21_menu}
		; service - zones
		dc.b "Zones        "
		dc.t {0200000h+SF_22}
		; service - outputs
		dc.b "Outputs      "
		dc.t {0300000h+SF_23}
SRV_24_bs:	; service - quick control
		dc.b "Quick control"
		dc.t {0480000h+SRV_24_menu}
		; service - EOL 1 resistor
 #if {typ_centrali lt 5}
		dc.b "Inp.Z1 number"
 #else
		dc.b "EOL 1 resist."
 #endif
		dc.t {0500000h+SF_25}
		; service - EOL 2 resistor
 #if {typ_centrali lt 5}
		dc.b "Inp.Z2 number"
 #else
		dc.b "EOL 2 resist."
 #endif
		dc.t {0600000h+SF_26}
 #if {typ_centrali eq 4}
		; service - Z3 zone number
		dc.b "Inp.Z3 number"
		dc.t {0700000h+SF_27}
		; service - Z4 zone number
		dc.b "Inp.Z4 number"
		dc.t {0800000h+SF_28}
 #endif
 #if {typ_centrali gt 5}
		; service - VERSA main panel zones
		dc.b "VERSA zones  "
		dc.t {0700000h+SF_27}
 #endif
		; service - end of menu
		dc.b 0
		dc.t SRV_2_bs


		dc.t 0
SRV_24_menu:	; service - quick 1#/1* control
		dc.b "Control 1#/1*"
		dc.t {0100000h+SF_241}
		; service - quick 2#/2* control
		dc.b "Control 2#/2*"
		dc.t {0200000h+SF_242}
		; service - quick 3#/3* control
		dc.b "Control 3#/3*"
		dc.t {0300000h+SF_243}
		; service - quick 4#/4* control
		dc.b "Control 4#/4*"
		dc.t {0400000h+SF_244}
		; service - quick 5#/5* control
		dc.b "Control 5#/5*"
		dc.t {0500000h+SF_245}
		; service - quick 6#/6* control
		dc.b "Control 6#/6*"
		dc.t {0600000h+SF_246}
		; service - quick 7#/7* control
		dc.b "Control 7#/7*"
		dc.t {0700000h+SF_247}
		; service - quick 8#/8* control
		dc.b "Control 8#/8*"
		dc.t {0800000h+SF_248}
		; service - quick 9#/9* control
		dc.b "Control 9#/9*"
		dc.t {0900000h+SF_249}
		; service - quick 0#/0* control
		dc.b "Control 0#/0*"
		dc.t {0000000h+SF_240}
		; service - end of menu
		dc.b 0
		dc.t SRV_24_bs


		dc.t 0
SRV_21_menu:	; service - expanders identification
		dc.b "Identificat. "
		dc.t {0100000h+SF_211}
		; service - expanders settings
		dc.b "Settings     "
		dc.t {0200000h+SF_212}
SRV_213_bs:	; service - ACU-100 menu
		dc.b "Wireless dev."
		dc.t {0300000h+SF_213}
		; service - options
		dc.b "Options      "
		dc.t {0400000h+SF_214}
		; service - remove ABAX devices
		dc.b "Rem.ABAX dev."
		dc.t {0700000h+SF_217}
		; service - remove ABAX key-fobs
		dc.b "Rem.ABAX kfbs"
		dc.t {0800000h+SF_218}
		; service - remove RX key-fobs
		dc.b "Rem.RX k-fobs"
		dc.t {0900000h+SF_219}
		; service - keypads addresses
		dc.b "Keypads addr."
		dc.t {0000000h+SF_210}
		; service - end of menu
		dc.b 0
		dc.t SRV_21_bs


		dc.t 0
SRV_213_menu:	; service - new ACU-100 device
		dc.b "New device   "
		dc.t {0100000h+SF_2131}
		; service - edit ACU-100 device
		dc.b "Config.device"
		dc.t {0200000h+SF_2132}
		; service - remove ACU-100 device
		dc.b "Remove device"
		dc.t {0300000h+SF_2133}
		; service - ACU-100 zones
		dc.b "Wirelss.zones"
		dc.t {0400000h+SF_2134}
		; service - perform synchronization
		dc.b "Synchronize  "
		dc.t {0500000h+SF_2135}
		; service - turn test mode on
		dc.b "Test mode on "
		dc.t {0600000h+SF_2136}
		; service - turn test mode on
		dc.b "Test mode off"
		dc.t {0700000h+SF_2137}
		; service - connecting message
		dc.b "Connect msg. "
		dc.t {0800000h+SF_2138}
		; service - end of menu
		dc.b 0
		dc.t SRV_213_bs


		dc.t 0
SRV_3_menu:	; service - options
		dc.b "Options     "
		dc.b 32
		dc.t {0100000h+SF_31}
		; service - Alarm time in keypads
		dc.b "Kpds al.time "
		dc.t {0200000h+SF_32}
		; service - suppress arm status time
		dc.b "Hide arm st. "
		dc.t {0300000h+SF_33}
		; service - Max. no AC time
		dc.b "AC trbl.delay"
		dc.t {0400000h+SF_34}
		; service - Max. no TL time
		dc.b "Tel.trbl.del."
		dc.t {0500000h+SF_35}
		; service - RCT clock adjustment
		dc.b "RTC adjustm. "
		dc.t {0600000h+SF_36}
		; service - Winter/summer time changing adjust
		dc.b "Daylight sav."
		dc.t {0700000h+SF_37}
		; service - Summer time begins
		dc.b "Summer time  "
		dc.t {0800000h+SF_38}
		; service - Winter time begins
		dc.b "Winter time  "
		dc.t {0900000h+SF_39}
		; service - Minimal code length
		dc.b "Min.code len."
		dc.t {0000000h+SF_30}
		; service - end of menu
		dc.b 0
		dc.t SRV_3_bs


		dc.t 0
SRV_4_menu:	; service - timer 1 name
		dc.b "Timer 1 name "
		dc.t {0100000h+SF_41}
		; service - timer 2 name
		dc.b "Timer 2 name "
		dc.t {0200000h+SF_42}
		; service - timer 3 name
		dc.b "Timer 3 name "
		dc.t {0300000h+SF_43}
		; service - timer 4 name
		dc.b "Timer 4 name "
		dc.t {0400000h+SF_44}
		; service - end of menu
		dc.b 0
		dc.t SRV_4_bs


		dc.t 0
SRV_7_menu:	; service - Rings to answer
		dc.b "Rings to ans."
		dc.t {0100000h+SF_71}
		; service - end of menu
		dc.b 0
		dc.t SRV_7_bs


		dc.t 0
SRV_8_menu:	; service - Template settings
		dc.b "Settings    "
		dc.b 32
		dc.t {0100000h+SF_81}
		; service - Template key fob
		dc.b "Key fob func."
		dc.t {0200000h+SF_82}
		; service - Template key fob confirmation
		dc.b "Confirmations"
		dc.t {0300000h+SF_83}
		; service - Template name
		dc.b "Name         "
		dc.t {0400000h+SF_84}
		; service - end of menu
		dc.b 0
		dc.t SRV_8_bs


		dc.t 0
SRV_5_menu:	; service - Monitoring station selection
 #if {TST_MAN eq 0}
		dc.b "Stations     "
		dc.t {0000000h+SF_50}
SRV_51_bs:	; service - Monitoring station 1
		dc.b "Station 1    "
		dc.t {0180000h+SRV_51_menu}
SRV_52_bs:	; service - Monitoring station 2
		dc.b "Station 2    "
		dc.t {0280000h+SRV_52_menu}
		; service - SIA options
		dc.b "SIA options "
		dc.b 32
		dc.t {0300000h+SF_53}
SRV_54_bs:	; service - Event codes
		dc.b "Event codes  "
		dc.t {0480000h+SRV_54_menu}
		; service - Test at
		dc.b "Test at      "
		dc.t {0500000h+SF_55}
		; service - Test every
		dc.b "Test every   "
		dc.t {0600000h+SF_56}
		; service - Test every (when armed)
		dc.b "Test (armed) "
		dc.t {0700000h+SF_57}
		; service - end of menu
		dc.b 0
		dc.t SRV_5_bs


		dc.t 0
SRV_51_menu:	; service - Tel. 1 number
		dc.b "Tel. number  "
		dc.t {0100000h+SF_511}
		; service - Tel. 1 format
		dc.b "Tel. format  "
		dc.t {0200000h+SF_512}
		; service - Options
		dc.b "Options     "
		dc.b 32
		dc.t {0300000h+SF_513}
		; service - Tries count
		dc.b "Attempts.no. "
		dc.t {0400000h+SF_514}
		; service - Suspension time
		dc.b "Suspens.time "
		dc.t {0500000h+SF_515}
SRV_516_bs:	; service - Identifiers
		dc.b "Identifiers  "
		dc.t {0680000h+SRV_516_menu}
		; service - TELIM/SIA prefix
		dc.b "T-M/SIA pref."
		dc.t {0700000h+SF_517}
		; service - TCP/IP monitoring settings
		dc.b "StationTCP/IP"
		dc.t {0800000h+SF_518}
		; service - SIA-IP acct
		dc.b "SIA-IP acct  "
		dc.t {0900000h+SF_519}
		; service - end of menu
		dc.b 0
		dc.t SRV_51_bs


		dc.t 0
SRV_516_menu:	; service - Identifier 1
		dc.b "Id.1         "
		dc.t {0100000h+SF_5161}
		; service - Identifier 2
		dc.b "Id.2         "
		dc.t {0200000h+SF_5162}
		; service - Identifier 3
		dc.b "Id.3         "
		dc.t {0300000h+SF_5163}
		; service - System identifier
		dc.b "System Id.   "
		dc.t {0000000h+SF_5160}
		; service - end of menu
		dc.b 0
		dc.t SRV_516_bs


		dc.t 0
SRV_52_menu:	; service - Tel. 2 number
		dc.b "Tel. number  "
		dc.t {0100000h+SF_521}
		; service - Tel. 2 format
		dc.b "Tel. format  "
		dc.t {0200000h+SF_522}
		; service - Options
		dc.b "Options     "
		dc.b 32
		dc.t {0300000h+SF_523}
		; service - Tries count
		dc.b "Attempts.no. "
		dc.t {0400000h+SF_524}
		; service - Suspension time
		dc.b "Suspens.time "
		dc.t {0500000h+SF_525}
SRV_526_bs:	; service - Identifiers
		dc.b "Identifiers  "
		dc.t {0680000h+SRV_526_menu}
		; service - TELIM/SIA prefix
		dc.b "T-M/SIA pref."
		dc.t {0700000h+SF_527}
		; service - TCP/IP monitoring settings
		dc.b "StationTCP/IP"
		dc.t {0800000h+SF_528}
		; service - SIA-IP acct
		dc.b "SIA-IP acct  "
		dc.t {0900000h+SF_529}
		; service - end of menu
		dc.b 0
		dc.t SRV_52_bs


		dc.t 0
SRV_526_menu:	; service - Identifier 1
		dc.b "Id.1         "
		dc.t {0100000h+SF_5261}
		; service - Identifier 2
		dc.b "Id.2         "
		dc.t {0200000h+SF_5262}
		; service - Identifier 3
		dc.b "Id.3         "
		dc.t {0300000h+SF_5263}
		; service - System identifier
		dc.b "System Id.   "
		dc.t {0000000h+SF_5260}
		; service - end of menu
		dc.b 0
		dc.t SRV_526_bs


		dc.t 0
SRV_54_menu:
SRV_541_bs:	; service - Partition 1 codes
		dc.b "Partition 1  "
		dc.t {0180000h+SRV_541_menu}
SRV_542_bs:	; service - Partition 2 codes
		dc.b "Partition 2  "
		dc.t {0280000h+SRV_542_menu}
SRV_543_bs:	; service - Zone codes
		dc.b "Zones        "
		dc.t {0380000h+SRV_543_menu}
SRV_544_bs:	; service - ABAX zone codes
		dc.b "Wirelss.zones"
		dc.t {0480000h+SRV_544_menu}
SRV_545_bs:	; service - Ekspander alarm codes
		dc.b "Exp. modules "
		dc.t {0580000h+SRV_545_menu}
SRV_546_bs:	; service - Ekspander supply codes
		dc.b "Exp. supply  "
		dc.t {0680000h+SRV_546_menu}
SRV_547_bs:	; service - System codes
		dc.b "System       "
		dc.t {0780000h+SRV_547_menu}
		; service - TELIM codes
		dc.b "TELIM codes  "
		dc.t {0000000h+SF_540}
		; service - end of menu
		dc.b 0
		dc.t SRV_54_bs


		dc.t 0
SRV_541_menu:	; service - Arm by user
		dc.b "Arm by user  "
		dc.t {0100000h+SF_5411}
		; service - Arm other
		dc.b "Arm other    "
		dc.t {0200000h+SF_5412}
		; service - Quick arm
		dc.b "Quick arm    "
		dc.t {0300000h+SF_5413}
		; service - Disarm by user
		dc.b "Disarm by usr"
		dc.t {0400000h+SF_5414}
		; service - Disarm other
		dc.b "Disarm other "
		dc.t {0500000h+SF_5415}
		; service - Clear by user
		dc.b "Rest.by user "
		dc.t {0600000h+SF_5416}
		; service - Clear other
		dc.b "Restore other"
		dc.t {0700000h+SF_5417}
		; service - Duress
		dc.b "Duress       "
		dc.t {0800000h+SF_5418}
		; service - Arming failed
		dc.b "Arming failed"
		dc.t {0900000h+SF_5419}
		; service - end of menu
		dc.b 0
		dc.t SRV_541_bs


		dc.t 0
SRV_542_menu:	; service - Arm by user
		dc.b "Arm by user  "
		dc.t {0100000h+SF_5421}
		; service - Arm other
		dc.b "Arm other    "
		dc.t {0200000h+SF_5422}
		; service - Quick arm
		dc.b "Quick amr    "
		dc.t {0300000h+SF_5423}
		; service - Disarm by user
		dc.b "Disarm by usr"
		dc.t {0400000h+SF_5424}
		; service - Disarm other
		dc.b "Disarm other "
		dc.t {0500000h+SF_5425}
		; service - Clear by user
		dc.b "Rest.by user "
		dc.t {0600000h+SF_5426}
		; service - Clear other
		dc.b "Restore other"
		dc.t {0700000h+SF_5427}
		; service - Duress
		dc.b "Duress       "
		dc.t {0800000h+SF_5428}
		; service - Arming failed
		dc.b "Arming failed"
		dc.t {0900000h+SF_5429}
		; service - end of menu
		dc.b 0
		dc.t SRV_542_bs


		dc.t 0
SRV_543_menu:	; service - Zone alarm
		dc.b "Alarm        "
		dc.t {0100000h+SF_5431}
		; service - Zone restore
		dc.b "Alarm restore"
		dc.t {0200000h+SF_5432}
		; service - Zone tamper
		dc.b "Tamper       "
		dc.t {0300000h+SF_5433}
		; service - Zone tamper restore
		dc.b "Tmp restore  "
		dc.t {0400000h+SF_5434}
		; service - Zone trouble
		dc.b "Trouble      "
		dc.t {0500000h+SF_5435}
		; service - Zone trouble restore
		dc.b "Trouble rest."
		dc.t {0600000h+SF_5436}
		; service - Zone bypass
		dc.b "Bypass       "
		dc.t {0700000h+SF_5437}
		; service - Zone unbypass
		dc.b "Unbypass     "
		dc.t {0800000h+SF_5438}
		; service - end of menu
		dc.b 0
		dc.t SRV_543_bs


		dc.t 0
SRV_544_menu:	; service - Zone communication trouble
		dc.b "Commun. loss "
		dc.t {0100000h+SF_5441}
		; service - Zone communication restore
		dc.b "Commun. rst. "
		dc.t {0200000h+SF_5442}
		; service - Zone battery low
		dc.b "Battery low  "
		dc.t {0300000h+SF_5443}
		; service - Zone battery restore
		dc.b "Battery rst. "
		dc.t {0400000h+SF_5444}
		; service - end of menu
		dc.b 0
		dc.t SRV_544_bs


		dc.t 0
SRV_545_menu:	; service - Expander tamper
		dc.b "Tamper       "
		dc.t {0100000h+SF_5451}
		; service - Expander tamper restore
		dc.b "Tmp restore  "
		dc.t {0200000h+SF_5452}
		; service - Fire alarm
		dc.b "Fire alarm   "
		dc.t {0300000h+SF_5453}
		; service - Medical alarm
		dc.b "Medical alarm"
		dc.t {0400000h+SF_5454}
		; service - Panic alarm
		dc.b "Panic alarm  "
		dc.t {0500000h+SF_5455}
		; service - 3 wrong codes
		dc.b "3 wrong codes"
		dc.t {0600000h+SF_5456}
		; service - 3 wrong cards
		dc.b "3 wrong cards"
		dc.t {0700000h+SF_5457}
		; service - end of menu
		dc.b 0
		dc.t SRV_545_bs


		dc.t 0
SRV_546_menu:	; service - Expander AC trouble
		dc.b "AC trouble   "
		dc.t {0100000h+SF_5461}
		; service - Expander AC restore
		dc.b "AC restore   "
		dc.t {0200000h+SF_5462}
		; service - Expander DC trouble
		dc.b "Batt. trouble"
		dc.t {0300000h+SF_5463}
		; service - Expander DC restore
		dc.b "Batt. restore"
		dc.t {0400000h+SF_5464}
		; service - Expander supply output overload
		dc.b "Overload     "
		dc.t {0500000h+SF_5465}
		; service - Expander supply output ok
		dc.b "Overload rst."
		dc.t {0600000h+SF_5466}
		; service - end of menu
		dc.b 0
		dc.t SRV_546_bs


		dc.t 0
SRV_547_menu:	; service - Troubles
		dc.b "Troubles     "
		dc.t {0100000h+SF_5471}
		; service - Troubles restore
		dc.b "Troubles rst."
		dc.t {0200000h+SF_5472}
		; service - Other
		dc.b "Other        "
		dc.t {0300000h+SF_5473}
		; service - RTC setting
		dc.b "RTC setting  "
		dc.t {0400000h+SF_5474}
		; service - end of menu
		dc.b 0
		dc.t SRV_547_bs
 #endif


		dc.t 0
SRV_6_menu:	; service - Messaging zone alarms
		dc.b "Zone alarms  "
		dc.t {0100000h+SF_61}
		; service - Messaging output starts
		dc.b "Output trig. "
		dc.t {0200000h+SF_62}
SRV_63_bs:	; service - Messaging arming
		dc.b "Arming       "
		dc.t {0380000h+SRV_63_menu}
SRV_64_bs:	; service - Messaging disarming
		dc.b "Disarming    "
		dc.t {0480000h+SRV_64_menu}
SRV_65_bs:	; service - Messaging other sources
		dc.b "Other        "
		dc.t {0580000h+SRV_65_menu}
SRV_66_bs:	; service - Messaging type
		dc.b "Message type "
		dc.t {0680000h+SRV_66_menu}
SRV_67_bs:	; service - Messaging PAGER parameters
		dc.b "PAGER param. "
		dc.t {0780000h+SRV_67_menu}
		; service - Messaging queue/try count
		dc.b "Queues/tries "
		dc.t {0800000h+SF_68}
		; service - Messaging messages
		dc.b "Messages     "
		dc.t {0900000h+SF_69}
		; service - Messaging telephones
		dc.b "Telephones   "
		dc.t {0000000h+SF_60}
		; service - end of menu
		dc.b 0
		dc.t SRV_6_bs


		dc.t 0
SRV_63_menu:	; service - partition 1 by user
		dc.b "Part.1 user  "
		dc.t {0100000h+SF_631}
		; service - partition 1 others
		dc.b "Part.1 other "
		dc.t {0200000h+SF_632}
		; service - partition 2 by user
		dc.b "Part.2 user  "
		dc.t {0300000h+SF_633}
		; service - partition 2 others
		dc.b "Part.2 other "
		dc.t {0400000h+SF_634}
		; service - arming partition 1 failed
		dc.b "Arm.p1 failed"
		dc.t {0500000h+SF_635}
		; service - arming partition 2 failed
		dc.b "Arm.p2 failed"
		dc.t {0600000h+SF_636}
		; service - end of menu
		dc.b 0
		dc.t SRV_63_bs


		dc.t 0
SRV_64_menu:	; service - partition 1 by user
		dc.b "Part.1 user  "
		dc.t {0100000h+SF_641}
		; service - partition 1 others
		dc.b "Part.1 other "
		dc.t {0200000h+SF_642}
		; service - partition 2 by user
		dc.b "Part.2 user  "
		dc.t {0300000h+SF_643}
		; service - partition 2 others
		dc.b "Part.2 other "
		dc.t {0400000h+SF_644}
		; service - end of menu
		dc.b 0
		dc.t SRV_64_bs


		dc.t 0
SRV_65_menu:	; service - tamper alarm
		dc.b "Tamper alarm "
		dc.t {0100000h+SF_651}
		; service - tamper restore
		dc.b "Tamper rest. "
		dc.t {0200000h+SF_652}
		; service - AC trouble
		dc.b "AC trouble   "
		dc.t {0300000h+SF_653}
		; service - AC restore
		dc.b "AC restore   "
		dc.t {0400000h+SF_654}
		; service - akku trouble
		dc.b "Battery trbl."
		dc.t {0500000h+SF_655}
		; service - akku restore
		dc.b "Battery rest."
		dc.t {0600000h+SF_656}
		; service - tel. line restore
		dc.b "Tel.lin.rest."
		dc.t {0700000h+SF_657}
		; service - end of menu
		dc.b 0
		dc.t SRV_65_bs


		dc.t 0
SRV_66_menu:	; service - Messaging type for tel. 1
		dc.b "Tel1 msg.type"
		dc.t {0100000h+SF_661}
		; service - Messaging type for tel. 2
		dc.b "Tel2 msg.type"
		dc.t {0200000h+SF_662}
		; service - Messaging type for tel. 3
		dc.b "Tel3 msg.type"
		dc.t {0300000h+SF_663}
		; service - Messaging type for tel. 4
		dc.b "Tel4 msg.type"
		dc.t {0400000h+SF_664}
		; service - Messaging type for tel. 5
		dc.b "Tel5 msg.type"
		dc.t {0500000h+SF_665}
		; service - Messaging type for tel. 6
		dc.b "Tel6 msg.type"
		dc.t {0600000h+SF_666}
		; service - Messaging type for tel. 7
		dc.b "Tel7 msg.type"
		dc.t {0700000h+SF_667}
		; service - Messaging type for tel. 8
		dc.b "Tel8 msg.type"
		dc.t {0800000h+SF_668}
		; service - end of menu
		dc.b 0
		dc.t SRV_66_bs


		dc.t 0
SRV_67_menu:	; service - Messaging PAGER 1 parameters
		dc.b "PAGER 1      "
		dc.t {0100000h+SF_671}
		; service - Messaging PAGER 2 parameters
		dc.b "PAGER 2      "
		dc.t {0200000h+SF_672}
		; service - end of menu
		dc.b 0
		dc.t SRV_67_bs


UF_sap_list:	dc.b "Permanent access"
		dc.b "Edit users      "
		dc.b "Arm/Dis/Clr/Bps "


sm_06_list:	dc.b "SrvMod via RESET"


SRV_txt_id:	dc.b "Change ID ?     "
		dc.b "           1=Yes"


SRV_07_txt:	dc.b "Restore factory "
		dc.b "settings ? 1=Yes"


 #if {typ_centrali lt 5}
SRV_07_e:	dc.b "Restore ETH mod."
		dc.b "settings ? 1=Yes"
 #endif


SRV_08_txt:	dc.b "Restore factory "
		dc.b "users ?    1=Yes"


 #if {typ_centrali ne 4}
SRV_09_txt1:	dc.b "Run updating    "
		dc.b "program on PC..."

SRV_09_txt2:	dc.b "STARTER         "
		dc.b "started...      "
 #endif


SRV_del_txt:	dc.b "Remove ?        "
		dc.b "           1=Yes"


SRV_210_txt:	dc.b "This KPD address"

SRV_210_nfo:	dc.b "Keypads address "
		dc.b "setting...      "


sm_17_lst:	dc.b "P1 infin.ex.time"
		dc.b "P2 infin.ex.time"
		dc.b "P1 timer prior. "
		dc.b "P2 timer prior. "
		dc.b "P1 simpl.defer. "
		dc.b "P2 simpl.defer. "
		dc.b "P1 singl.defer. "
		dc.b "P2 singl.defer. "
		dc.b "P1 en.tim.in day"
		dc.b "P2 en.tim.in day"


sm_214_list:	dc.b "Grade2          "
		dc.b "Arm ExDly w.trbl"
		dc.b "Advanced arming "


sm_31_list:	dc.b "TEL. reporting  "
		dc.b "ETHM-1 reporting"
		;;; dc.b "SMS reporting   "
		dc.b "Tel.messaging   "
		dc.b "Modem answering "
		dc.b "Double call     "
		dc.b "Tone dialing    "
		dc.b "Puls.dial. 1/1.5"
		dc.b "No dial tone tst"
		dc.b "No answer test  "
		dc.b "PC-16 OUT       "
		dc.b "PC-16 OUT UA    "
TX_trbls_m:	dc.b "Troubles memory "
		dc.b "Sign.from z.only"
		dc.b "Entry err. warn."
		dc.b "EntrErr int.sir."
		dc.b "Ans. if P1 armed"
		dc.b "Ans. if P2 armed"
		dc.b "Autoabort mess. "
		dc.b "Tmp.always loud "
		dc.b "Tmp.on int.siren"
		dc.b "TMP alarm in P.2"
		dc.b "Key-fob events  "
		dc.b "Block.on 3wrong "
		dc.b "Events limitat. "
		dc.b "Exp.restart.rep."
		dc.b "Rest.aft. bell  "
		dc.b "Rest.aft. disarm"
		dc.b "Test ev. limit. "
		dc.b "Mess.aft.tamper "


FS_ETopt_list:	dc.b "DHCP            "
		dc.b "DHCP-DNS        "
		dc.b 68,76,79,65,68,88,Arr_right,69,84,72,77,45,49,32,32,32
		dc.b "SATEL server LAN"
 #if {typ_centrali eq 4}
  #if {VeIP eq 0}
		dc.b "USSD - any tel. "
  #endif
		dc.b "Use ETHM        "
  #if {VeIP eq 0}
		dc.b "Use SIM1        "
		dc.b "Use SIM2        "
  #endif
 #endif
		dc.b "Mobile app.     "
		dc.b "Time from srvLAN"
 #if {typ_centrali eq 4}
  #if {VeIP eq 0}
   #if {version_low gt '6'}
		dc.b "SATEL server GSM"
		dc.b "Time from srvGSM"
   #endif
  #endif
 #endif
		dc.b "PUSH messages   "


sm_37_list:	dc.b "No time change  "
		dc.b "UE standard     "
		dc.b "US standard     "
		dc.b "1h by dates     "
		dc.b "2h by dates     "
sm_37_cnt	equ {{$-sm_37_list}/16}


sm_51_days:	dc.b "Monday   ON/OFF"
		dc.b 32
		dc.b "Tuesday  ON/OFF"
		dc.b 32
		dc.b "Wednesd. ON/OFF"
		dc.b 32
		dc.b "Thursday ON/OFF"
		dc.b 32
		dc.b "Friday   ON/OFF"
		dc.b 32
		dc.b "Saturday ON/OFF"
		dc.b 32
		dc.b "Sunday   ON/OFF"
		dc.b 32
		dc.b "Everyday ON/OFF"
		dc.b 32


sm_52_days:	dc.b "Except.  ON/OFF"
		dc.b 32


sm_81_list:	dc.b "Arm             "
		dc.b "Disarm          "
		dc.b "Clear alarm     "
		dc.b "Abort messaging "
		dc.b "Deferr. autoarm "
		dc.b "Zones inhibit   "
		dc.b "Zones isolate   "
		dc.b "Change own code "
		dc.b "Users           "
		dc.b "Control         "
		dc.b "Settings        "
		dc.b "DOWNLOAD/SERV.  "
		dc.b "Events          "
		dc.b "Tests           "
		dc.b "DURESS          "
		dc.b "INT-VG          "


SRV_69_txt:	dc.b "Voice msg.num. "
		dc.b 32


SRV_60_txt:	dc.b "Telephon.# name"
		dc.b 32


SRV_222_txt:	dc.b "EOL type       "
		dc.b 32

sf222_list:	dc.b "0.Not used      "
		dc.b "1.EOL=0 (NC)    "
		dc.b "2.EOL=0 (NO)    "
		dc.b "3.EOL=1         "
		dc.b "4.EOL=2 (NC)    "
		dc.b "5.EOL=2 (NO)    "
		dc.b "6.Roller        "
		dc.b "7.Vibration     "
sf222_cnt	equ {{$-sf222_list}/16}


SRV_224_txt:	dc.b "Time frame     "
		dc.b 32


SRV_228_txt:	dc.b "Type           "
		dc.b 32

sf228_list:	dc.b "0.Entry/Exit    "
		dc.b "1.En/Ex final   "
		dc.b "2.En/Ex route   "
		dc.b "3.Instant       "
		dc.b "4.Double knock  "
		dc.b "5.24h burglary  "
		dc.b "6.24h tamper    "
		dc.b "7.24h panic     "
		dc.b "8.24h panic sil."
		dc.b "9.24h medical   "
		dc.b "10.24h fire     "
		dc.b "11.Det. mask    "
		dc.b "12.No alarm act."
		dc.b "13.Arm/disarm   "
		dc.b "14.Arming       "
		dc.b "15.Disarming    "
		dc.b "16.Ex.dly term. "
		dc.b "17.Shunt lock   "
		dc.b "18.En.rout.enbl."
		dc.b "19.Trouble      "
sf228_cnt	equ {{$-sf228_list}/16}


SRV_229_amtxt:	dc.b "Arm mode       "
		dc.b 32


SRV_229_txt:	dc.b "Alarm delay    "
		dc.b 32


SRV_22A_txt:	dc.b "Max.viol.time  "
		dc.b 32


SRV_22B_txt:	dc.b "Z.inactiv.time "
		dc.b 32


SRV_22C_list:	dc.b "Al.on exit end  "
		dc.b "Priority        "
		dc.b "Bypass disabled "
		dc.b "Active night arm"
		dc.b "Active day arm  "
		dc.b "Power up delay  "
		dc.b "Warn.in part.arm"
		dc.b "Warn.on int.sir."
		dc.b "Auto-bypass 3   "
		dc.b "Auto-bypass 1   "
		dc.b "Autobypass reset"
		dc.b "Arm.with one p. "
		dc.b "Disable verific."
		dc.b "Finish exit time"


SRV_22D_txt:	dc.b "Zone ## name   "
		dc.b 32

SRV_22E_txt:	dc.b "Exp.## name    "
		dc.b 32


SRV_231_txt:	dc.b "Function       "
		dc.b 32

sf231_list:	dc.b "0.Not used      "
		dc.b "1.External siren"
		dc.b "2.Internal siren"
		dc.b "3.Burglary alarm"
		dc.b "4.Fire alarm    "
		dc.b "5.Duress alarm  "
		dc.b "6.Panic alarm   "
		dc.b "7.Medical alarm "
		dc.b "8.Unverified al."
		dc.b "9.Verified alarm"
		dc.b "10.Tamper alarm "
		dc.b "11.Supply fire  "
		dc.b "12.Supply armed "
		dc.b "13.Zone violat. "
		dc.b "14.Chime        "
		dc.b "15.Control      "
		dc.b "16.READY status "
		dc.b "17.Exit delay s."
		dc.b "18.Armed status "
		dc.b "19.Trouble stat."
		dc.b "20.Al/arm status"
		dc.b "21.Zones reset  "
 #if {version_low gt '5'}
		dc.b "22.ETHGSM trbls."
 #endif
sf231_cnt	equ {{$-sf231_list}/16}


SRV_232_txt:	dc.b "Cut-off time   "
		dc.b 32


SRV_234n_list:	dc.b "Part.1 clears   "
		dc.b "Part.2 clears   "
		dc.b "Pulsation       "
		dc.b "Polarization +  "
		dc.b "Fire alarm      "
		dc.b "Arm/dArm/Cl.chrp"
		dc.b "Part.1 alarms   "
		dc.b "Part.2 alarms   "
		dc.b "31.TMP zone     "


SRV_235_txt:	dc.b "Output ## name "
		dc.b 32


 #if {typ_centrali lt 5}
SRV_236_txt:	dc.b "Sound type     "
		dc.b 32
 #endif


SRV_211_txt_1:	dc.b "Wrong exp.addr.:"

SRV_211_txt_2:	dc.b "Multiple expand."
		dc.b "with address ## "

SRV_211_txt_3:	dc.b "## expanders    "
		dc.b "found (## new)  "


FS_exp_strefa:	dc.b "Tamper in p.## "
		dc.b 32


FS_lcd_chime:	dc.b "Zone chime    "
		dc.b 32


FS_lcd_wy:	dc.b "Outputs       "
		dc.b 32


FS_lcd_format:	dc.b "Time format    "
		dc.b 32

TX_lcdfmt_list:	dc.b "           hh:mm"
		dc.b "        hh:mm:ss"
		dc.b "dd mmm yy, hh:mm"
		dc.b "dd mmm, hh:mm:ss"
		dc.b " yy-mm-dd, hh:mm"
		dc.b "yyyy-mm-dd,hh:mm"
		dc.b "ddd dd mmm,hh:mm"
		dc.b "keypad name     "
TX_lcdfmt_cnt	equ {{$-TX_lcdfmt_list}/16}


FS_lig_lcd:	dc.b "LCD backlight  "
		dc.b 32

TX_liglcd_list:	dc.b "             off"
		dc.b "             50%"
		dc.b "            100%"
		dc.b "   auto  0 - 50%"
		dc.b "  auto  0 - 100%"
		dc.b " auto  50 - 100%"
TX_liglcd_cnt	equ {{$-TX_liglcd_list}/16}


FS_lig_key:	dc.b "Kpd. backlight "
		dc.b 32

TX_ligkey_list:	dc.b "             off"
		dc.b "            auto"
		dc.b "       permanent"
TX_ligkey_cnt	equ {{$-TX_ligkey_list}/16}


FS_aulig1:	dc.b "Auto backlight "
		dc.b 32

TX_aulig1_list:	dc.b "off             "
		dc.b "zone violation  "
		dc.b "entry delay     "
TX_aulig1_cnt	equ {{$-TX_aulig1_list}/16}


FS_vol:		dc.b "Volume         "
		dc.b 32

FS_volchime:	dc.b "Chime volume   "
		dc.b 32

FS_volTwe:	dc.b "Entry time vol."
		dc.b 32

FS_volTwy:	dc.b "Exit time vol. "
		dc.b 32

FS_volfire:	dc.b "Fire alarm vol."
		dc.b 32

FS_volalarm:	dc.b "Alarm volume   "
		dc.b 32

FS_volwarn:	dc.b "Warn.alarm vol."
		dc.b 32

FS_voltrbl:	dc.b "Troubles volume"
		dc.b 32


FS_Lop_list:	dc.b "Entry time sign."
		dc.b "Exit time sign. "
		dc.b "Alarm signalling"
		dc.b "Part.1 QuickArm "
		dc.b "Part.2 QuickArm "
		dc.b "Key sounds      "
		dc.b "Trbl.in part.arm"
		dc.b "Code entry ind. "
		dc.b "Chime on/off    "
		dc.b "Quick control   "
		dc.b "New trbl.signal."
		dc.b "Autoarm signal. "
		dc.b "Prox.card - arms"
		dc.b "Arm mode check. "
		dc.b "Photo frame     "


FS_mcuop_list:	dc.b "Presence control"
sm_wyb_tit:	dc.b "Wake up        ",32
		dc.b "Card reader     "

sm_wyb_list:	dc.b "status          "
		dc.b "menu            "
		dc.b "disarming       "
sm_wyb_cnt	equ {{$-sm_wyb_list}/16}


FS_lcdal:	dc.b "Alarms        "
		dc.b 32

FS_lcdal_list:	dc.b "Fire alarm      "
		dc.b "Medical alarm   "
		dc.b "Panic alarm     "
		dc.b "Silent panic    "
		dc.b "3 wrong codes   "
		dc.b "Part.alarm msg. "
		dc.b "Zone alarm msg. "


FS_lcdname:	dc.b "Exp.## name    "
		dc.b 32


FS_txm_to:	dc.b "BUSY filtr.time"
		dc.b 32


FS_acu_okres:	dc.b "Polling period "
		dc.b 32


FS_acu_opt:	dc.b "Jam sensitivity "
		dc.b "Usr.replaces BAT"


TX_options:	dc.b "Options       "
		dc.b 32


FS_CA64i_EOL1:	dc.b "EOL 1 resist.  "
		dc.b 32


FS_CA64i_EOL2:	dc.b "EOL 2 resist.  "
		dc.b 32


FS_CA64i_AC:	dc.b "AC loss delay  "
		dc.b 32


FS_IT_FxSx:	dc.b "LED # - part.# "
		dc.b 32


TX_Arms_list:	dc.b "Does not arm    "
Nm_QA1:		dc.b "Full arm        "
Nm_QA2:		dc.b "Stay night arm  "
Nm_QA3:		dc.b "Stay day arm    "
		dc.b "Disarm          "
Nm_NotArmed:	dc.b "Not armed       "
Nm_EntryTime:	dc.b "Entry time      "
Nm_ExitTime:	dc.b "Exit time       "


FS_IT_list:	dc.b "Timed alarm sign"
		dc.b "Alm.until clear "
		dc.b "3 wrng cards al."
		dc.b "Entry time sign."
		dc.b "Exit time sign. "
		dc.b "Hardware signal."


SRV_42_2_txt:	dc.b "Exception start"
		dc.b 32
SRV_42_3_txt:	dc.b "Exception end  "
		dc.b 32


sm_70_list:	dc.b "0.Station 1 or 2"
		dc.b "1.Station 1     "
		dc.b "2.Station 2     "
		dc.b "3.Station 1 & 2 "
sm_70_cnt	equ {{$-sm_70_list}/16}


sm_7_2_list:	dc.b "0.Silent Knight "
		dc.b "1.Sescoa/Vertex "
		dc.b "2.S.Knight Fast "
		dc.b "3.Radionics 1400"
		dc.b "4.Radionics 2300"
		dc.b "5.Radion. p.1400"
		dc.b "6.Radion. p.2300"
		dc.b "7.Ademco Express"
		dc.b "8.S.Knight ext. "
		dc.b "9.Sescoa/V. ext."
		dc.b "A.S.Knigh.F.ext."
		dc.b "B.Radion.1400ext"
		dc.b "C.Radion.2300ext"
		dc.b "D.TELIM         "
		dc.b "E.CID selected  "
		dc.b "F.CID all       "
		dc.b "G.SIA selected  "
		dc.b "H.SIA all       "
sm_7_2_cnt	equ {{$-sm_7_2_list}/16}


sm_7_3_list:	dc.b "GuardTone(TELIM)"
		dc.b "Ext.handsh.await"
		dc.b "Extended kissoff"


sm_73_list:	dc.b "MS1 ident. ack. "
		dc.b "MS2 ident. ack. "
		dc.b "MS1 blocks. ack."
		dc.b "MS2 blocks. ack."
		dc.b "MS1 source name "
		dc.b "MS2 source name "
		dc.b "MS1 part. name  "
		dc.b "MS2 part. name  "


sm_mety_list:	dc.b "no messaging    "
		dc.b "1.PAGER 1       "
		dc.b "2.PAGER 2       "
		dc.b "3.Voice         "
		dc.b "4.SMS           "


TX_wait:	dc.b "Please wait...  "
		dc.b "                "


STD_zone:	dc.b "Zone ##       "
		dc.b 32,32
STD_zone31:	dc.b "Zone TMP      "
		dc.b 32,32

KPD_output:	dc.b "KPD output      "

AUX_output:	dc.b "AUX output      "

PVR_output:	dc.b "+VR output      "

STD_output:	dc.b "Output ##     "
		dc.b 32,32

STD_part:	dc.b "Partition##    "		; no space before ## - the 1st # will be replaced by space
		dc.b 32

STD_exp:	dc.b "Expander     ",35,35
		dc.b 32

STD_timer:	dc.b "Timer##        "		; no space before ## - the 1st # will be replaced by space
		dc.b 32

STD_telPwd:	dc.b "Telephone##    "		; no space before ## - the 1st # will be replaced by space
		dc.b 32

STD_komun:	dc.b "Message ##      "

STD_user:	dc.b "User ##         "

STD_serv:	dc.b "Service         "

STD_TIMER:	dc.b "TIMER           "

STD_ZONE:	dc.b "ZONE            "

STD_sch:	dc.b "Normal          "
		dc.b "Simple          "
		dc.b "Arms only       "
		dc.b "Duress          "
		dc.b "Master          "

Nm_DURESS:	dc.b "DURESS          "

Nm_ArmFail:	dc.b "Arming failed   "

Nm_sysKD:	dc.b "AC 230V trouble "
		dc.b "Battery trouble "
		dc.b "CLK/DAT trouble "
		dc.b "ABAX jamming    "
		dc.b "MS1 trouble     "
		dc.b "MS2 trouble     "
		dc.b "OUT1 overload   "
		dc.b "OUT2 overload   "
		dc.b "KPD overload    "
		dc.b "AUX overload    "
 #if {typ_centrali eq 4}
		dc.b "+VR overload    "
 #else
		dc.b "Not used        "
 #endif
		dc.b "Not used        "
		dc.b "Tel.line trouble"
		dc.b "No LAN cable    "

Nm_RsysKD:	dc.b "230V mains rest."
		dc.b "Battery rest.   "
		dc.b "CLK/DAT rest.   "
		dc.b "ABAX jam.rest.  "
		dc.b "MS1 restore     "
		dc.b "MS2 restore     "
		dc.b "OUT1 ovl.restore"
		dc.b "OUT2 ovl.restore"
		dc.b "KPD ovl.restore "
		dc.b "AUX ovl.restore "
 #if {typ_centrali eq 4}
		dc.b "+VR ovl.restore "
 #else
		dc.b "Not used        "
 #endif
		dc.b "Not used        "
		dc.b "Tel.line restore"
		dc.b "LAN cable rest. "

Nm_OsysKD:	dc.b "Memory error    "
		dc.b "Panel restart   "
		dc.b "Service restart "
		dc.b "Callback        "
		dc.b "DWNL successful "
		dc.b "DWNL unsuccessf."
		dc.b "Periodic test   "
		dc.b "RTC trouble     "
		dc.b "Serv.Mode start "
		dc.b "Serv.Mode end   "
		dc.b "Verified alarm  "
		dc.b "DLOADX started  "
		dc.b "Time set. DLOADX"
		dc.b "Autoarm defer.  "

Nms_TELIMKD:	dc.b "Code # (#)      "


SRV_6x_txt:	dc.b "Msg.destination"
		dc.b 32

FT_mess_prm:	dc.b "M/T"			; i.e. Message/Telephones
		dc.b 58,32,35,35,32,35,35,35,35,35,35,35,35


TX_il_impulsow:	dc.b "Pulses count   "
		dc.b 32

TX_czulosc:	dc.b "Sensitivity    "
		dc.b 32


TX_abax_ov:	dc.b "No free space   "

TX_sn:		dc.b "Serial number  "
		dc.b 32

TX_abax_tmp:	dc.b "Open device     "
		dc.b "####### tamper  "

TX_abax_alrd:	dc.b "Device #######  "
		dc.b "already logged  "

TX_abax_add:	dc.b "           1=Add"

TX_abax_chn:	dc.b "Channels ? "
		dc.b 40,49,45,50,41

TX_abax_del:	dc.b "Remove ?   1=Yes"
		dc.b 63,63,63,63,63,63,63,32

BX_filtr:	dc.b "Filter         "
		dc.b 32

BX_aktywnosc:	dc.b "Active mode    "
BX_akty_list:	dc.b "always active   "

BX_asd_list:	dc.b "alarm from other"
		dc.b "broadcasts alarm"

BX_czulosc_PIR:	dc.b "PIR sensitivity"
		dc.b 32

BX_czulosc_MW:	dc.b "MW sensitivity "
		dc.b 32

BX_czulosc_DN:	dc.b "DN sensitivity "
		dc.b 32

BX_animal:	dc.b "Animal resist  "

BX_apmd_test:	dc.b "Test           "
		dc.b 32

BX_sound_type:	dc.b "Sound type     "
		dc.b 32

BX_sound_time:	dc.b "Sound duration "
		dc.b 32

BX_a100:	dc.b "Button         "
		dc.b 32

BX_a100_l_lst:	dc.b "inactive        "
		dc.b "interim control "
		dc.b "combined control"
BX_a100_l_cnt	equ {{$-BX_a100_l_lst}/16}

BX_flash:	dc.b "Flash          "
BX_flash_list:	dc.b "active          "

BX_magn_test:	dc.b "Magnet. contact"
		dc.b 32

BX_magn_list:	dc.b "bottom          "
		dc.b "side            "

BX_det_class:	dc.b "Detection class"
		dc.b 32

BX_detC_list0:	dc.b "no detection    "

BX_amd102_imp:	dc.b "Time frame     "
		dc.b 32

BX_impT_list3:	dc.b "no limit        "


TX_KPD_sp_over:	dc.b "Stack           "
		dc.b "overflow !!! (*)"

TX_no_QCnotlwd:	dc.b "Quick control   "
		dc.b "unavailable     "

TX_osrtd:	dc.b "Outputs         "
		dc.b "switched        "

TX_no_out2ctrl:	dc.b "No output       "
		dc.b "to control      "

TX_outctrl_off:	dc.b "Turned OFF:     "

TX_outctrl_on:	dc.b "Turned ON:      "

TX_disarmed:	dc.b "Disarmed        "
TX_cleared:	dc.b "Alarm cleared   "
TX_mess_abort:	dc.b "Messag. aborted "
TX_armed:	dc.b "Armed           "
TX_rearmed:	dc.b "Arm mode changed"

TX_SrvAcc:	dc.b "Service access "
		dc.b 32

TX_SerAcc:	dc.b "Access changed  "

 #if {typ_centrali lt 5}
TX_dwnlrs_st:	dc.b "USBcomm started "

TX_dwnlrs_fn:	dc.b "USBcomm end     "
 #else
TX_dwnlrs_st:	dc.b "RScomm started  "

TX_dwnlrs_fn:	dc.b "RScomm end      "
 #endif

TX_dwnlethm_st:	dc.b "Commun. started "

TX_code:	dc.b "New code       "
		dc.b 32

TX_codeOK:	dc.b "Code changed    "


TX_RTC_1:	dc.b "Enter time     "
		dc.b 32

TX_RTC_2:	dc.b "Enter date     "
		dc.b 32

TX_RTCOK:	dc.b "RTC clock set   "

TX_TELOK:	dc.b "Tel. changed    "

TX_abort_msg:	dc.b "V.msg. aborted  "


TX_enter_code:	dc.b 0
		dc.b "Enter code      "


TX_choose:	dc.b "CHOOSE      "
		dc.b 40,Arr_up,Arr_down,41

TX_nothing:	dc.b "no action       "


RX_RBT_txt:	dc.b "Buttn.$ fun.###"
		dc.b 32


RX_BTN_tbl:	dc.b   0,"not used        "
		dc.b  31,"Arm part.1 full "
		dc.b  32,"Arm part.1 night"
		dc.b  33,"Arm part.1 day  "
		dc.b  34,"Dis/Clr part.1  "
		dc.b  35,"Arm part.2 full "
		dc.b  36,"Arm part.2 night"
		dc.b  37,"Arm part.2 day  "
		dc.b  38,"Dis/Clr part.2  "
		dc.b  39,"Arm p.1&2 full  "
		dc.b  40,"Arm p.1&2 night "
		dc.b  41,"Arm p.1&2 day   "
		dc.b  42,"Dis/Clr part.1&2"
		dc.b  43,"Panic alarm     "
		dc.b  44,"Silent panic    "
		dc.b  45,"Fire alarm      "
		dc.b  46,"Medical alarm   "
		dc.b 255			; 255 - koniec tabeli


AB_LED_cnf:	dc.b "LED $ conf.### "
		dc.b 32

ABLED_0:	dc.b "Light on        "

ABLED_13_26:	dc.b "Part.1 armed    "
		dc.b "Part.2 armed    "
		dc.b "Part.1or2 armed "
		dc.b "Part.1 & 2 armed"
		dc.b "P.1 full armed  "
		dc.b "P.1 night armed "
		dc.b "P.1 day armed   "
		dc.b "P.2 full armed  "
		dc.b "P.2 night armed "
		dc.b "P.2 day armed   "
		dc.b "Part.1 alarm    "
		dc.b "Part.2 alarm    "
		dc.b "Part. 1or2 alarm"
		dc.b "Trouble         "


TX_telnr:	dc.b "Tel. number    "
		dc.b 32

TX_edtuser:	dc.b "Edit user ##   "
		dc.b 32

TX_remuser:	dc.b "Remove user ## "
		dc.b 32

TX_bypass:	dc.b "Zone ## bypass"
		dc.b 32

TX_bpsOK:	dc.b "End of bypasses "


RSN_we_viol:	dc.b "Zone ## violat.:"

RSN_more:	dc.b "And more...     "
		dc.b "                "

TX_rsns_bps:	dc.b "Bypass ?   1=Yes"


TX_violzns:	dc.b "Violated zones  "

TX_arm_bps:	dc.b "Bypassed zones  "
		dc.b "1=Arm 4=Bypasses"

TX_trbls:	dc.b "Troubles        "

TX_no_trbls:	dc.b "No troubles     "

TX_arm:		dc.b 0
		dc.b "1=Arm           "

TX_arm_check:	dc.b 0
		dc.b "1=Arm 2=Check   "


TX_ok_check:	dc.b 0
		dc.b "1=Ok 2=Check    "

TX_ok_bps:	dc.b "Bypassed zones  "
		dc.b "1=Ok 4=Bypasses "


TX_inv_msg:	dc.b "Connecting...   "


RESTORE		equ 00400h

EVENTS_tbl:	dc.w {0010000000000000b+UF_Password}
		dc.b "Code change     "

		dc.w {0010100000000000b+UF_Bypass}
		dc.b "Zone bypasses   "

		dc.w {0010000000000000b+UF_TSpermit}
		dc.b "Permit service  "

		dc.w {0010000000000000b+UF_TSpermit+RESTORE}
		dc.b "Disable service "

		dc.w {0010000000000000b+UF_NewUserBy}
		dc.b "User addition   "

		dc.w {0010000000000000b+UF_NewUserWho}
		dc.b "New user        "

		dc.w {0010000000000000b+UF_EditUserBy}
		dc.b "User edition    "

		dc.w {0010000000000000b+UF_EditUserWho}
		dc.b "Edited user     "

		dc.w {0010000000000000b+UF_DelUserBy}
		dc.b "User removal    "

		dc.w {0010000000000000b+UF_DelUserWho}
		dc.b "Removed user    "

		dc.w {0010000000000000b+UF_DwnlRS}
 #if {typ_centrali lt 5}
		dc.b "USB-DWNL started"
 #else
		dc.b "RS-DWNL started "
 #endif

		dc.w {0010000000000000b+UF_MS_1}
		dc.b "Station 1 test  "

		dc.w {0010000000000000b+UF_MS_2}
		dc.b "Station 2 test  "

		dc.w {0000000000000000b+UF_FlashProgram}
		dc.b "Firmware updated"

		dc.w {0000000000000000b+UF_Starter}
		dc.b "STARTER started "

		dc.w {0010000000000000b+UF_DwnlRS+RESTORE}
 #if {typ_centrali lt 5}
		dc.b "USB-DWNL finish."
 #else
		dc.b "RS-DWNL finished"
 #endif

		dc.w {0010000000000000b+UF_KasPowTelExp}
		dc.b "Voice m. aborted"

		dc.w {0000000000000000b+UF_TimeToSummer}
		dc.b "Summer time     "

		dc.w {0000000000000000b+UF_TimeToWinter}
		dc.b "Winter time     "

		dc.w {0001100000000000b+UF_WarnAlarm}
		dc.b "Warning alarm   "

		dc.w {0010100000000000b+UF_ClrWarnAl}
		dc.b "Warn.al.cleared "

		dc.w {0000000000000000b+UF_TCP_DX_conn}
		dc.b "St.TCP/IP DLOADX"

		dc.w {0000000000000000b+UF_TCP_DX_conn+RESTORE}
		dc.b "En.TCP/IP DLOADX"

		dc.w {0000000000000000b+UF_TCP_DX_crack}
		dc.b "?? TCP/IP DLOADX"

		dc.w {0001100000000000b+UF_Bps_Keys}
		dc.b "Kpd temp.blocked"

		dc.w {0001100000000000b+UF_Bps_Reader}
		dc.b "Rdr temp.blocked"

		dc.w {0000000000000000b+UF_NewRTC}
		dc.b "RTC clock set   "

		dc.w {0010000000000000b+UF_TrblClr}
		dc.b "Trbl.mem.cleared"

		dc.w {0000000000000000b+78}
		dc.b "No network (LAN)"

		dc.w {0000000000000000b+78+RESTORE}
		dc.b "Network ok (LAN)"

		dc.w {0000000000000000b+82}
		dc.b "Msg. confirmed  "

		dc.w {0001100000000000b+UF_BadCodes}
		dc.b "3 wrong codes   "

		dc.w {0000000000000000b+88}
		dc.b "GSM trouble     "

		dc.w {0000000000000000b+88+RESTORE}
		dc.b "End of GSM trbl."

		dc.w {0000000000000000b+UF_EndOfWFDWNL}
		dc.b "End of DWNL rdy."

		dc.w {0000000000000000b+UF_StartDWNL}
		dc.b "DWNL started    "

		dc.w {0001100000000000b+UF_ExpAbsent}
		dc.b "Mod.tamper (pre)"

		dc.w {0001100000000000b+UF_ExpAbsent+RESTORE}
		dc.b "Module ok (pre) "

		dc.w {0001100000000000b+UF_ExpTMP}
		dc.b "Mod.tamper (TMP)"

		dc.w {0001100000000000b+UF_ExpTMP+RESTORE}
		dc.b "Module ok (TMP) "

		dc.w {1000000000000000b+UF_OutOV}
		dc.b "Overload        "

		dc.w {1000000000000000b+UF_OutOV+RESTORE}
		dc.b "Overload restore"

		dc.w {0001100000000000b+UF_LongViol}
		dc.b "Long violation  "

		dc.w {0001100000000000b+UF_LongViol+RESTORE}
		dc.b "Long viol. rest."

		dc.w {0001100000000000b+UF_NoViol}
		dc.b "No violation    "

		dc.w {0001100000000000b+UF_NoViol+RESTORE}
		dc.b "Violat. present "

		dc.w {0001100000000000b+UF_Violation}
		dc.b "Zone violation  "

		dc.w {0001100000000000b+UF_Violation+RESTORE}
		dc.b "Zone restore    "

		dc.w {0010100000000000b+UF_ArmAborted}
		dc.b "Arming aborted  "

		dc.w {0010100000000000b+UF_SirenClear}
		dc.b "Sounder off     "

		dc.w {0010100000000000b+UF_ArmStart_usr}
		dc.b "Exit time startd"

		dc.w {0000000000000000b+UF_SMS_ctrl}
		dc.b "SMS control     "

		dc.w {0000000000000000b+UF_SMS_empty}
		dc.b "SMS no control  "

		dc.w {0000000000000000b+UF_SMS_unauth}
		dc.b "SMS unauthorized"

		dc.w {0010000000000000b+UF_Pilot}
		dc.b "Key fob used    "

		dc.w {0001100000000000b+100}
		dc.b "Medic. request  "

		dc.w {0001100000000000b+100+RESTORE}
		dc.b "Med.request rst."

		dc.w {0001100000000000b+110}
		dc.b "Fire alarm      "

		dc.w {0001100000000000b+110+RESTORE}
		dc.b "Fire alarm rest."

		dc.w {0010100000000000b+121}
		dc.b "Duress alarm    "

		dc.w {0001100000000000b+122}
		dc.b "Silent panic    "

		dc.w {0001100000000000b+122+RESTORE}
		dc.b "Silnt.panic rst."

		dc.w {0001100000000000b+123}
		dc.b "Audible panic   "

		dc.w {0001100000000000b+123+RESTORE}
		dc.b "Audbl.panic.rst."

		dc.w {0001100000000000b+130}
		dc.b "Burglary alarm  "

		dc.w {0001100000000000b+130+RESTORE}
		dc.b "Burgl.al.restore"

		dc.w {0001100000000000b+132}
		dc.b "Alarm interior  "

		dc.w {0001100000000000b+132+RESTORE}
		dc.b "Interior restore"

		dc.w {0001100000000000b+133}
		dc.b "Alarm 24h burgl."

		dc.w {0001100000000000b+133+RESTORE}
		dc.b "24h burgl. rest."

		dc.w {0001100000000000b+134}
		dc.b "Alarm exit/entry"

		dc.w {0001100000000000b+134+RESTORE}
		dc.b "Exit/entry rest."

		dc.w {0001100000000000b+137}
		dc.b "Al. tamp. perim."

		dc.w {0001100000000000b+137+RESTORE}
		dc.b "Tamp.perim.rest."

		dc.w {0001100000000000b+139}
		dc.b "Verified alarm  "

		dc.w {0000100000000000b+143}
		dc.b "Al.-DTA line tr."

		dc.w {0000100000000000b+143+RESTORE}
		dc.b "DTA line ok     "

		dc.w {0001100000000000b+144}
		dc.b "Zone tamper     "

		dc.w {0001100000000000b+144+RESTORE}
		dc.b "Zone tamp. rest."

		dc.w {0001100000000000b+151}
		dc.b "Gas detected    "

		dc.w {0001100000000000b+151+RESTORE}
		dc.b "Rest.gas detect."

		dc.w {0001100000000000b+152}
		dc.b "Refrigeration   "

		dc.w {0001100000000000b+152+RESTORE}
		dc.b "Rest.refrigerat."

		dc.w {0001100000000000b+153}
		dc.b "Loss of heat    "

		dc.w {0001100000000000b+153+RESTORE}
		dc.b "Rest. heat loss "

		dc.w {0001100000000000b+154}
		dc.b "Water leakage   "

		dc.w {0001100000000000b+154+RESTORE}
		dc.b "Rest.water leak."

		dc.w {0001100000000000b+155}
		dc.b "Foil break      "

		dc.w {0001100000000000b+155+RESTORE}
		dc.b "Rest.foil break "

		dc.w {0001100000000000b+156}
		dc.b "Day trouble     "

		dc.w {0001100000000000b+156+RESTORE}
		dc.b "Rest.day trouble"

		dc.w {0001100000000000b+157}
		dc.b "Low gas level   "

		dc.w {0001100000000000b+157+RESTORE}
		dc.b "Rest.low gas lvl"

		dc.w {0001100000000000b+158}
		dc.b "High temp.      "

		dc.w {0001100000000000b+158+RESTORE}
		dc.b "Rest. high temp."

		dc.w {0001100000000000b+159}
		dc.b "Low temp.       "

		dc.w {0001100000000000b+159+RESTORE}
		dc.b "Rest. low temp. "

		dc.w {0001100000000000b+161}
		dc.b "Loss of air flow"

		dc.w {0001100000000000b+161+RESTORE}
		dc.b "Rest. air flow  "

		dc.w {0001100000000000b+162}
		dc.b "CO detected     "

		dc.w {0001100000000000b+162+RESTORE}
		dc.b "Rest. CO detect."

		dc.w {0001100000000000b+163}
		dc.b "Tank level      "

		dc.w {0001100000000000b+163+RESTORE}
		dc.b "Rest. tank level"

		dc.w {0001100000000000b+201}
		dc.b "Low water press."

		dc.w {0001100000000000b+201+RESTORE}
		dc.b "Rest.water pres."

		dc.w {0001100000000000b+202}
		dc.b "Low CO2         "

		dc.w {0001100000000000b+202+RESTORE}
		dc.b "Rest. low CO2   "

		dc.w {0001100000000000b+203}
		dc.b "Gate valve sens."

		dc.w {0001100000000000b+203+RESTORE}
		dc.b "Rest.valve sens."

		dc.w {0001100000000000b+204}
		dc.b "Low water level "

		dc.w {0001100000000000b+204+RESTORE}
		dc.b "Rest. low water "

		dc.w {0001100000000000b+205}
		dc.b "Pump activated  "

		dc.w {0001100000000000b+205+RESTORE}
		dc.b "Rest.pump activ."

		dc.w {0001100000000000b+206}
		dc.b "Pump failure    "

		dc.w {0001100000000000b+206+RESTORE}
		dc.b "Rest. pump fail."

		dc.w {0001100000000000b+220}
		dc.b "Keybox open     "

		dc.w {0001100000000000b+220+RESTORE}
		dc.b "Keybox restore  "

		dc.w {0001100000000000b+301}
		dc.b "No AC (230V)    "

		dc.w {0001100000000000b+301+RESTORE}
		dc.b "AC (230V) ok    "

		dc.w {0001100000000000b+302}
		dc.b "Battery low     "

		dc.w {0001100000000000b+302+RESTORE}
		dc.b "Battery ok      "

		dc.w {0000000000000000b+303}
		dc.b "RAM memory error"

		dc.w {0001100000000000b+305}
		dc.b "M.panel restart "

		dc.w {0001100000000000b+312}
		dc.b "Overload        "

		dc.w {0001100000000000b+312+RESTORE}
		dc.b "Overload restore"

		dc.w {0010000000000000b+313}
		dc.b "Engineer reset  "

		dc.w {0001100000000000b+330}
		dc.b "Mod.tamper (pre)"

		dc.w {0001100000000000b+330+RESTORE}
		dc.b "Module ok (pre) "

		dc.w {0001100000000000b+333}
		dc.b "DTA line trouble"

		dc.w {0001100000000000b+333+RESTORE}
		dc.b "DTA line ok     "

		dc.w {0001100000000000b+338}
		dc.b "Module batt. low"

		dc.w {0001100000000000b+338+RESTORE}
		dc.b "Module batt. ok "

		dc.w {0001100000000000b+339}
		dc.b "Module restart  "

		dc.w {0001100000000000b+341}
		dc.b "Module tamper   "

		dc.w {0001100000000000b+341+RESTORE}
		dc.b "Module tamp.rst."

		dc.w {0001100000000000b+342}
		dc.b "No mod.AC (230V)"

		dc.w {0001100000000000b+342+RESTORE}
		dc.b "Mod.AC (230V) ok"

		dc.w {0001100000000000b+344}
		dc.b "Jam detected    "

		dc.w {0001100000000000b+344+RESTORE}
		dc.b "Jam ended       "

		dc.w {0000000000000000b+350}
		dc.b "Monitoring trbl."

		dc.w {0000000000000000b+350+RESTORE}
		dc.b "Monitoring ok   "

		dc.w {0000000000000000b+351}
		dc.b "Tel.line trouble"

		dc.w {0000000000000000b+351+RESTORE}
		dc.b "Tel.line ok     "

		dc.w {0001100000000000b+373}
		dc.b "Fire zone tamper"

		dc.w {0001100000000000b+373+RESTORE}
		dc.b "Fire zone t.rst."

		dc.w {0001100000000000b+380}
		dc.b "Zone trb.(mask.)"

		dc.w {0001100000000000b+380+RESTORE}
		dc.b "Zone ok (mask.) "

		dc.w {0001100000000000b+381}
		dc.b "Radio conn.trbl."

		dc.w {0001100000000000b+381+RESTORE}
		dc.b "Radio conn. ok  "

		dc.w {0001100000000000b+383}
		dc.b "Zone trb.(tamp.)"

		dc.w {0001100000000000b+383+RESTORE}
		dc.b "Zone tamp. rest."

		dc.w {0001100000000000b+384}
		dc.b "Radio batt. low "

		dc.w {0001100000000000b+384+RESTORE}
		dc.b "Radio batt. ok  "

		dc.w {0010100000000000b+401}
		dc.b "Disarm          "

		dc.w {0010100000000000b+401+RESTORE}
		dc.b "Arm             "

		dc.w {0000100000000000b+403}
		dc.b "Auto-disarm     "

		dc.w {0000100000000000b+403+RESTORE}
		dc.b "Auto-arm        "

		dc.w {0010100000000000b+406}
		dc.b "Alarm cleared   "

		dc.w {0100100000000000b+408+RESTORE}
		dc.b "Quick arm       "

		dc.w {0001100000000000b+409}
		dc.b "Disarm by zone  "

		dc.w {0001100000000000b+409+RESTORE}
		dc.b "Arm by zone     "

		dc.w {0000000000000000b+411}
		dc.b "Callback made   "

		dc.w {0000000000000000b+412}
		dc.b "DWNL finished   "

		dc.w {0000000000000000b+413}
		dc.b "Unsucc.rem. DWNL"

		dc.w {0010100000000000b+441+RESTORE}
		dc.b "Arm (STAY)      "

		dc.w {0010100000000000b+442+RESTORE}
		dc.b "Arm (STAY) by z."

		dc.w {0010100000000000b+454}
		dc.b "Arming failed   "

		dc.w {0001100000000000b+458}
		dc.b "Delay activ.time"

		dc.w {0001100000000000b+461}
		dc.b "Al.-3 wrong cod."

		dc.w {0010100000000000b+464}
		dc.b "Autoarm deferred"

		dc.w {0001100000000000b+570}
		dc.b "Zone bypass     "

		dc.w {0001100000000000b+570+RESTORE}
		dc.b "Zone unbypass   "

		dc.w {0001100000000000b+575}
		dc.b "Auto.byps.(viol)"

		dc.w {0001100000000000b+575+RESTORE}
		dc.b "Auto.ubps.(viol)"

		dc.w {0010000000000000b+601}
		dc.b "Manual tran.test"

		dc.w {0000000000000000b+602}
		dc.b "Transmiss. test "

		dc.w {0010100000000000b+607}
		dc.b "Zones test      "

		dc.w {0010100000000000b+607+RESTORE}
		dc.b "Zones test end  "

		dc.w {0000000000000000b+608}
		dc.b "Trns.test(trbl.)"

		dc.w {0010000000000000b+625}
		dc.b "Time setting    "

		dc.w {0000000000000000b+626}
		dc.b "RTC trouble     "

		dc.w {0001000000000000b+627}
		dc.b "Service start   "

		dc.w {0001000000000000b+628}
		dc.b "Service end     "

		dc.w {0001000000000000b+979}
		dc.b "MAC/ID error    "

		dc.w {0001000000000000b+979+RESTORE}
		dc.b "MAC/ID ok       "

		dc.w {0001000000000000b+980}
		dc.b "No conn.SATELsrv"

		dc.w {0001000000000000b+980+RESTORE}
		dc.b "SATELsrv conn.ok"

		dc.w {0010000000000000b+988}
		dc.b "Mob.app.-conect."

		dc.w {0010000000000000b+988+RESTORE}
		dc.b "Mob.app.-discon."

		dc.w {0010000000000000b+989}
		dc.b "Log in  (INT-VG)"

		dc.w {0010000000000000b+989+RESTORE}
		dc.b "Log out (INT-VG)"

		dc.w {0001100000000000b+991}
		dc.b "Auto.byps.(tamp)"

		dc.w {0001100000000000b+991+RESTORE}
		dc.b "Auto.ubps.(tamp)"

		dc.w {0010000000000000b+UF_ConfTRBL}
		dc.b "Confirm.troubles"

		dc.w {0010000000000000b+UF_ConfBatRX}
		dc.b "Cfmd.low.RX kf. "

		dc.w {0010000000000000b+UF_ConfBatABAX}
		dc.b "Cfmd.low.ABAX kf"

		dc.w {0010000000000000b+UF_LowRX}
		dc.b "Low RX kf.bat.  "

		dc.w {0010000000000000b+UF_LowABAX}
		dc.b "Low ABAX kf.bat."

		dc.w {0001000000000000b+997}
		dc.b "Long BUSY state "

		dc.w {0001000000000000b+997+RESTORE}
		dc.b "End of long BUSY"

		dc.w {0010100000000000b+1001}
		dc.b "Forced arming   "

		dc.w {0000000000000000b+1002}
		dc.b "No network(PING)"

		dc.w {0000000000000000b+1002+RESTORE}
		dc.b "Network ok(PING)"

		dc.w {0010000000000000b+1005}
		dc.b "DWNL-ETH start  "

		dc.w {0001000000000000b+1020}
		dc.b "ETHM1 init.error"

		dc.w {0001000000000000b+1020+RESTORE}
		dc.b "ETHM1 init. ok  "

		dc.w 0
