awarie_s:	dc.b "System AC      "
		dc.b "(230V) trouble  "

		dc.b "No system      "
		dc.b "battery         "

		dc.b "System battery "
		dc.b "trouble         "

		dc.b "No voltage on  "
		dc.b "telephone line  "

CME_unknown:	dc.b "GSM SIM#       "
		dc.b "error (####)    "

ind_alert:	dc.b "Information    "
		dc.b "for other users "

		dc.b "KPD supply     "
		dc.b "trouble         "

		dc.b "AUX supply     "
		dc.b "trouble         "

awaria_ping:	dc.b "No network     "
		dc.b "(PING test)     "

awaria_lan:	dc.b "No LAN cable   "
		dc.b "                "

		dc.b "No tone on     "
		dc.b "telephone line  "

		dc.b "Broken tone on "
		dc.b "telephone line  "

		dc.b "ABAX jamming   "
		dc.b "                "

		dc.b "DTA data bus   "
		dc.b "trouble         "

		dc.b "System RTC     "
		dc.b "clock trouble   "

		dc.b "Settings memory"
		dc.b "trouble         "

		dc.b "Panel          "
		dc.b "restart         "

		dc.b "HSE circuit    "
		dc.b "trouble         "

		dc.b "+VR supply     "
		dc.b "trouble         "

		dc.b "GSM jamming    "
		dc.b "                "

		dc.b "Long busy state"
		dc.b "in transmitter  "

 #if {typ_centrali eq 4}
		dc.b "VERSA-ETH      "
		dc.b "initiation error"
 #else
		dc.b "ETHM-1         "
		dc.b "initiation error"
 #endif

 #if {typ_centrali eq 2}
		dc.b "NiMH battery   "
		dc.b "unchargeable    "

		dc.b "NiMH battery   "
		dc.b "discharges fast "
 #endif

awaria_mon:	dc.b "No connection  "
		dc.b "with MS# (TEL)  "

awaria_STLlack:	dc.b "No connection  "
		dc.b "with SATEL serv."

awaria_STLerr:	dc.b "Error of MAC/ID"
		dc.b "for SATEL server"

awaria_out:	dc.b "OUT# trouble  "
		dc.b 32

TST_no_data:	dc.b 0
		dc.b "NO DATA AVAIL.  "

		segment 'data'		;!!! Do NOT translate this line !!!

awaria_E_mon:	dc.b "Monitor.trouble"
		dc.b 32
		dc.b "station"
		dc.b 32

awaria_E_pin:	dc.b "Wrong PIN code "
		dc.b "(SIM# card) ",32,32,32,32

awaria_ZNtamp:	dc.b "Zone ## tamper"
		dc.b 32

awaria_ZNlong:	dc.b "Zn.## long v. "
		dc.b 32

awaria_ZNlack:	dc.b "Zn.## no viol."
		dc.b 32

awaria_ZNtmpV:	dc.b "Viol.tamp.z.##"
		dc.b 32

awaria_ZNtmpT:	dc.b "Trouble zone##"
		dc.b 32

awaria_ZNmask:	dc.b "Zone ## masked"
		dc.b 32

awaria_EXPtmp:	dc.b "Exp.## tamper "
		dc.b 32

awaria_EXPlack:	dc.b "No expander ##"
		dc.b 32

awaria_EXPnoAC:	dc.b "No AC exp.##  "
		dc.b 32

awaria_EXPnAKU:	dc.b "No batb.exp.##"
		dc.b 32

awaria_EXPlAKU:	dc.b "Bat.trb.exp.##"
		dc.b 32

awaria_EXPlAC:	dc.b "AC trbl.exp.##"
		dc.b 32

awaria_EXPovr:	dc.b "Overload exp##"
		dc.b 32

awaria_USRkfR:	dc.b "U.## low RX   "
		dc.b 32

awaria_USRkfA:	dc.b "U.## low ABAX "
		dc.b 32

awaria_KPDbatt:	dc.b "Low BT# in ex#"
		dc.b 32

awaria_BXbatt:	dc.b "Z.## low batt."
		dc.b 32

awaria_BXlack:	dc.b "No zone ##    "
		dc.b 32

awaria_BXsync:	dc.b "Synchronization"
		dc.b "trouble (ABAX)  "

awaria_EXPrst:	dc.b "Exp.## restart"
		dc.b 32


TX_clr_trbls:	dc.b "Clear trouble   "
		dc.b "memory ?   1=Yes"

TX_hse_trbls:	dc.b "Make VERSA panel"
		dc.b "restart ?  1=Yes"

TX_view_clrd:	dc.b "View cleared    "
		dc.b "zones ?    1=Yes"


TX_Low_RX:	dc.b "Low RX key-fob  "
		dc.b "battery.    1=Ok"

TX_Low_ABAX:	dc.b "Low ABAX key-fob"
		dc.b "battery.    1=Ok"


EVN_eoevs:	dc.b "End of events   "
		dc.b "                "

TX_IP_addr:	dc.b "IP address:     "

EVN_unknown:	dc.b "UNKNOWN   "
		dc.b 32,32,32,32,32,32

EVN_TIMER:	dc.b "TIMER           "

EVN_ZONE:	dc.b "CONTROL ZONE    "


TX_alarm_aux:	dc.b "Medical alarm   "
		dc.b "activated       "

TX_alarm_fire:	dc.b "Fire alarm      "
		dc.b "activated       "

TX_alarm_panic:	dc.b "Panic alarm     "
		dc.b "activated       "

TX_gong_on:	dc.b "Keypad chime    "
		dc.b "active          "

TX_gong_off:	dc.b "Keypad chime    "
		dc.b "inactive        "


SW_AlarmINH:	dc.b "Z.## inhibited"
		dc.b 32

SW_AlarmISO:	dc.b "Z.## isolated "
		dc.b 32


SW_AlarmZone:	dc.b "Zone ## alarm  "
		dc.b 32
		dc.b "ZONE ## ALARM  "
		dc.b 32

SW_FireZone:	dc.b "Zone ## fire   "
		dc.b 32
		dc.b "ZONE ## FIRE   "
		dc.b 32

SW_AlarmPart:	dc.b "Part.# alarm   "
		dc.b 32

SW_FirePart:	dc.b "Part.# fire    "
		dc.b 32

SW_TampPart:	dc.b "Part.# tamper  "
		dc.b 32

SW_AutoTime:	dc.b "To autoarm "
		dc.b 32

SW_EntryTime:	dc.b "To entry   "
		dc.b 32

SW_ExitTime:	dc.b "To exit    "
		dc.b 32

SW_Service:	dc.b "System tamper,  "
		dc.b "call service    "


TX_fun_def:	dc.b "Autoarm deferred"


TST_wejsc:	dc.b "Test period    "
		dc.b 32


TST_abax_lvl:	dc.b "Signal z.##"
		dc.b 32,32,32,32

TST_abkp_lvl:	dc.b "Signal ex.#"
		dc.b 32,32,32,32


TST_trtst:	dc.b "Test event      "
		dc.b "added to log    "


TST_mstst_1:	dc.b "Waiting for     "
		dc.b "phone line free "

TST_mstst_dial:	dc.b "Dialing         "
		dc.b "                "

TST_mstst_hand:	dc.b "Waiting for     "
		dc.b "handshake       "

TST_mstst_dtmf:	dc.b "Sending         "
		dc.b "DTMF event      "

TST_mstst_ack:	dc.b "Waiting for     "
		dc.b "acknowledgement "

TST_mstst_puls:	dc.b "Sending         "
		dc.b "pulse event     "

TST_mstst_ext:	dc.b "Sending         "
		dc.b "extendend event "

TST_mstst_tlm:	dc.b "Sending         "
		dc.b "TELIM event     "

TST_mstst_sia:	dc.b "Sending         "
		dc.b "SIA event       "

TST_msres_0:	dc.b "Event sent      "
		dc.b "                "

TST_msres_1:	dc.b "No signal       "
		dc.b "on phone line   "

TST_msres_24:	dc.b "Wrong signal    "
		dc.b "on phone line   "

TST_msres_3:	dc.b "Busy signal     "
		dc.b "on phone line   "

TST_msres_5:	dc.b "No monitoring   "
		dc.b "station answer  "

TST_msres_6:	dc.b "No handshake    "
		dc.b "                "

TST_msres_7:	dc.b "No              "
		dc.b "acknowledgement "

TST_msres_err:	dc.b "Unknown error   "
		dc.b "                "


TST_volt_lvl:	dc.b "Voltage:  "
		dc.b 32,32,32,32,32,32

TST_volt_lack:	dc.b "unkn. "

TX_no_function:	dc.b "No function     "
		dc.b "available now   "

TX_no_srv_accs:	dc.b "Service access  "
		dc.b "disabled        "

TX_make_ident:	dc.b "Invoke expanders"
		dc.b "identification  "

CME_table:	dc.w 00009h
		dc.b "GSM SIM# phone "
		dc.b "does not answer "
		;
		dc.w 00010h
		dc.b "No SIM# card   "
		dc.b "in SIM holder   "
		;
		dc.w 00012h
		dc.b "SIM# PUK code  "
		dc.b "required        "
		;
		dc.w 00013h
		dc.b "SIM# card      "
		dc.b "failure         "
		;
		dc.w 00019h
		dc.b "No GSM SIM#    "
		dc.b "signal          "
		;
		dc.w 0

TX_funtimer:	dc.b "What to change "
		dc.b 32

TX_funti_list:	dc.b "Week schedule   "
		dc.b "Exception 1     "
		dc.b "Exception 2     "
		dc.b "Exception 3     "
		dc.b "Exception 4     "
TX_arm1mode:	dc.b "Part.1 arm mode "
TX_arm2mode:	dc.b "Part.2 arm mode "
TX_funti_cnt	equ {{$-TX_funti_list}/16}

		segment 'rom_h'		;!!! Do NOT translate this line !!!

fit_E_stacja:	dc.b "Station #"
		dc.b 32

SW_Synchro:	dc.b "Synchronization "
		dc.b "(ABAX system)..."
